<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-AIE8&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-04&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AIE8_35X45(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X45(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_35X50(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X50(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_22X35(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X35(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_30X45(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X45(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_35X35(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X35(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_22X45(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt;  Aluminum Electrolytic Capacitors,22X45(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_25X25(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt;  Aluminum Electrolytic Capacitors,25X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_35X30(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_30X30(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_30X35(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt;Aluminum Electrolytic Capacitors,30X35(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_22X40(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X40(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_25X40(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt;  Aluminum Electrolytic Capacitors,25X40(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_30X25(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_35X40(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt;Aluminum Electrolytic Capacitors,35X40(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_25X30(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt;  Aluminum Electrolytic Capacitors,25X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_22X30(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_30X40(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X40(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_35X25(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_22X25(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIE8_25X35(DXL)">
<description>&lt;B&gt;WCAP-AIE8&lt;/B&gt;&lt;BR&gt;  Aluminum Electrolytic Capacitors,25X35(DiameterXLength)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AIE8_35X50" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_35X50(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221486024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221486024.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1505.99uA"/>
<attribute name="I-RIPPLE" value="2880mA"/>
<attribute name="L" value="50mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221486024 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ500561M450DSIC2C000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_35X45" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_35X45(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221486023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221486023.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1379.67uA"/>
<attribute name="I-RIPPLE" value="2680mA"/>
<attribute name="L" value="45mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221486023 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ450471M450DSIC2C000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_30X45" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_30X45(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221485018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221485018.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1256.78uA"/>
<attribute name="I-RIPPLE" value="2350mA"/>
<attribute name="L" value="45mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221485018 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP450391M450DSIC2C000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_22X35" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_22X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221483004.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="697.14uA"/>
<attribute name="I-RIPPLE" value="1070mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221483004 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN350121M450DSIC3C000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_35X35" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_35X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221386021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221386021.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1300.77uA"/>
<attribute name="I-RIPPLE" value="2510mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221386021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ350471M400DSIC2C000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_861221486021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221486021.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1156.07uA"/>
<attribute name="I-RIPPLE" value="2150mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221486021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ350331M450DSIC2C000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_22X45" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_22X45(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221483006.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="853.81uA"/>
<attribute name="I-RIPPLE" value="1320mA"/>
<attribute name="L" value="45mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221483006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN450181M450DSIC3C000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_25X25" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_25X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221084006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221084006.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="919.78uA"/>
<attribute name="I-RIPPLE" value="1950mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221084006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO250471M200DSIC3C000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_861221484007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221484007.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="636.4uA"/>
<attribute name="I-RIPPLE" value="970mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221484007 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO250101M450DSIC3C000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_30X35" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_30X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221485016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221485016.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1045.71uA"/>
<attribute name="I-RIPPLE" value="1890mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221485016 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP350271M450DSIC2C000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_35X30" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_35X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861220786020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861220786020.pdf"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1963.57uA"/>
<attribute name="I-RIPPLE" value="4440mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861220786020 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANBQ300682M063DSIC2C000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_861221486020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221486020.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1045.71uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221486020 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ300271M450DSIC2C000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_30X30" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_30X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861220785014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861220785014.pdf"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1632.45uA"/>
<attribute name="I-RIPPLE" value="3540mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861220785014 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANBP300472M063DSIC2C000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_861221385012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221385012.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="889.94uA"/>
<attribute name="I-RIPPLE" value="1660mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221385012 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP300221M400DSIC2C000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_861221485014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221485014.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="853.81uA"/>
<attribute name="I-RIPPLE" value="1450mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221485014 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP300181M450DSIC2C000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861221485015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221485015.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="943.93uA"/>
<attribute name="I-RIPPLE" value="1640mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221485015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP300221M450DSIC2C000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_22X40" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_22X40(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221483005.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="779.42uA"/>
<attribute name="I-RIPPLE" value="1180mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221483005 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN400151M450DSIC3C000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_25X40" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_25X40(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221084017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221084017.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="1341.64uA"/>
<attribute name="I-RIPPLE" value="3280mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221084017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO400102M200DSIC3C000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_861221484011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221484011.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="943.93uA"/>
<attribute name="I-RIPPLE" value="1590mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221484011 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO400221M450DSIC3C000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_30X25" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_30X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221485012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221485012.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="697.14uA"/>
<attribute name="I-RIPPLE" value="1120mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221485012 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP250121M450DSIC2C000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861221485013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221485013.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="779.42uA"/>
<attribute name="I-RIPPLE" value="1290mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221485013 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP250151M450DSIC2C000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_25X30" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_25X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861220784007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861220784007.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="1367.88uA"/>
<attribute name="I-RIPPLE" value="2740mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861220784007 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANBO300332M063DSIC3C000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_861221484008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221484008.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="697.14uA"/>
<attribute name="I-RIPPLE" value="1090mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221484008 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO300121M450DSIC3C000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861221484009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221484009.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="779.42uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221484009 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO300151M450DSIC3C000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_22X30" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_22X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221483003.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="636.4uA"/>
<attribute name="I-RIPPLE" value="950mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221483003 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN300101M450DSIC3C000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_30X40" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_30X40(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221485017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221485017.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1156.07uA"/>
<attribute name="I-RIPPLE" value="2120mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221485017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP400331M450DSIC2C000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_35X25" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_35X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221486019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221486019.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="943.93uA"/>
<attribute name="I-RIPPLE" value="1590mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221486019 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ250221M450DSIC2C000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_22X25" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_22X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221483001.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="524.79uA"/>
<attribute name="I-RIPPLE" value="710mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221483001 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN250680M450DSIC3C000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861221483002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221483002.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="576.28uA"/>
<attribute name="I-RIPPLE" value="860mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221483002 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN250820M450DSIC3C000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_35X40" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_35X40(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221486022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221486022.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1256.78uA"/>
<attribute name="I-RIPPLE" value="2380mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221486022 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ400391M450DSIC2C000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_25X35" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 50.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14718v209%20Family_WCAP-AIE8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIE8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIE8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_25X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221484010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861221484010.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="853.81uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861221484010 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO350181M450DSIC3C000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
