<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ASLI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ASLI_16X17(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X17X6.6(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_6.3X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X5.5X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_4X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,4X5.5X1(DiameterXLengthXPitch)</description>
</package>
<package name="WCAP-ASLI_12.5X14(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,12.5X14X4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_6.3X7.7(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X7.7X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_8X6.5(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X6.5X2.3(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_10X10.5(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X10.5X4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_8X10.5(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X10.5X3.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_6.3X6.1(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X6.1X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLI_5X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X5.5X1.4(DiameterXLengthXP)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ASLI_4X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_4X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080140001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080140001.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080140001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055220M6R3DVCTAB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080140002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080140002.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="79mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080140002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055270M6R3DVCTAB000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080140003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080140003.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="82mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080140003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055330M6R3DVCTAB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080140004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080140004.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="86mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080140004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055470M6R3DVCTAB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080240001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080240001.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080240001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055220M010DVCTAB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080240003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080240003.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080240003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055330M010DVCTAB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080340001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080340001.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080340001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055100M016DVCTAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080340002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080340002.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080340002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055150M016DVCTAB000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080340003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080340003.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3.52uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080340003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055220M016DVCTAB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080440001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080440001.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080440001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0556R8M025DVCTAB000"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080440002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080440002.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080440002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055100M025DVCTAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080540001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080540001.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080540001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0553R3M035DVCTAB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080540002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080540002.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080540002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0554R7M035DVCTAB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080540003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080540003.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="88mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080540003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0556R8M035DVCTAB000"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080540004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080540004.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3.5uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080540004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055100M035DVCTAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080640001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080640001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080640001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055010M050DVCTAB000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080640002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080640002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080640002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0552R2M050DVCTAB000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080640003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080640003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080640003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0553R3M050DVCTAB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080640004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080640004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080640004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0554R7M050DVCTAB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080740002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080740002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3000uA"/>
<attribute name="I-RIPPLE" value="1mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080740002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055R10M063DVCTAB000"/>
<attribute name="VALUE" value="0.1  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080740003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080740003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="2mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080740003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055R22M063DVCTAB000"/>
<attribute name="VALUE" value="0.22  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080740004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080740004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="3mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080740004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055R33M063DVCTAB000"/>
<attribute name="VALUE" value="0.33  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080740005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080740005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="4mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080740005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055R47M063DVCTAB000"/>
<attribute name="VALUE" value="0.47  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080740006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080740006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="7mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080740006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055010M063DVCTAB000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080740007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080740007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="11mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080740007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0552R2M063DVCTAB000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080840001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080840001.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="7mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080840001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055010M100DVCTAB000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_865081740001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081740001.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="7mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081740001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055010M080DVCTAB000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_16X17" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_16X17(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080163018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080163018.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="428.4uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080163018 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170682M6R3DVCTHB000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080263016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080263016.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080263016 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170472M010DVCTHB000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080363018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080363018.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080363018 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170332M016DVCTHB000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080463017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080463017.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080463017 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170222M025DVCTHB000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080563018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080563018.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="1250mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080563018 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170152M035DVCTHB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080663020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080663020.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080663020 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170102M050DVCTHB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080763016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080763016.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="296.1uA"/>
<attribute name="I-RIPPLE" value="630mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080763016 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170471M063DVCTHB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080863009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080863009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="150uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080863009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170151M100DVCTHB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_865081763010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081763010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081763010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170151M080DVCTHB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
<technology name="_865081763011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081763011.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="176uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081763011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170221M080DVCTHB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_6.3X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_6.3X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080143008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080143008.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="9.45uA"/>
<attribute name="I-RIPPLE" value="235mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080143008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055151M6R3DVCTBB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080143009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080143009.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080143009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055221M6R3DVCTBB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080243005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080243005.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="5.6uA"/>
<attribute name="I-RIPPLE" value="210mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080243005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055560M010DVCTBB000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080243006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080243006.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="6.8uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080243006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055680M010DVCTBB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080243007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080243007.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080243007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055101M010DVCTBB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080243008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080243008.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="250mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080243008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055151M010DVCTBB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080343005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080343005.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="185mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080343005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055330M016DVCTBB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080343007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080343007.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="8.96uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080343007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055560M016DVCTBB000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080343008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080343008.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="10.88uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080343008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055680M016DVCTBB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080343009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080343009.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="255mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080343009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055101M016DVCTBB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080443005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080443005.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="6.75uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080443005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055270M025DVCTBB000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080443007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080443007.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080443007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055470M025DVCTBB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080443008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080443008.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="14uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080443008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055560M025DVCTBB000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080443009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080443009.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="17uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080443009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055680M025DVCTBB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080543007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080543007.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="9.45uA"/>
<attribute name="I-RIPPLE" value="210mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080543007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055270M035DVCTBB000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080543008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080543008.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080543008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055330M035DVCTBB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080543009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080543009.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080543009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055470M035DVCTBB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080643007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080643007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="7.5uA"/>
<attribute name="I-RIPPLE" value="140mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080643007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055150M050DVCTBB000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080643008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080643008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080643008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055220M050DVCTBB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080743010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080743010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="40mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080743010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055100M063DVCTBB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080843002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080843002.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="13mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080843002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED0552R2M100DVCTBB000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_865081743003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081743003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081743003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED0553R3M080DVCTBB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
<technology name="_865081743004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081743004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3.76uA"/>
<attribute name="I-RIPPLE" value="25mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081743004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED0554R7M080DVCTBB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_12.5X14" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_12.5X14(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080162017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080162017.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="207.9uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080162017 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140332M6R3DVCTGB000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080262015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080262015.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080262015 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140222M010DVCTGB000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080362017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080362017.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080362017 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140152M016DVCTGB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080462016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080462016.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080462016 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140102M025DVCTGB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080562016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080562016.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080562016 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140471M035DVCTGB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080562017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080562017.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080562017 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140681M035DVCTGB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080662019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080662019.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080662019 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140331M050DVCTGB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080762015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080762015.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="138.6uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080762015 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140221M063DVCTGB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080862008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080862008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080862008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140470M100DVCTGB000 ASEH140470M100DVCTGB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_865081762009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081762009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="I-LEAK" value="80uA"/>
<attribute name="I-RIPPLE" value="380mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081762009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140101M080DVCTGB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_6.3X7.7" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_6.3X7.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080145010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080145010.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="275mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080145010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077331M6R3DVCTCB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080245009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080245009.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080245009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077221M010DVCTCB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080345010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080345010.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="265mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080345010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077151M016DVCTCB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080345012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080345012.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="275mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080345012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077221M016DVCTCB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080445010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080445010.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="290mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080445010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077101M025DVCTCB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080545010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080545010.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.6uA"/>
<attribute name="I-RIPPLE" value="250mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080545010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077560M035DVCTCB000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080545011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080545011.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.8uA"/>
<attribute name="I-RIPPLE" value="265mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080545011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077680M035DVCTCB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080545012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080545012.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080545012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077101M035DVCTCB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080645009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080645009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.5uA"/>
<attribute name="I-RIPPLE" value="180mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080645009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077270M050DVCTCB000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080645010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080645010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="190mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080645010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077330M050DVCTCB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080645012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080645012.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080645012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077470M050DVCTCB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080745011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080745011.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080745011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077220M063DVCTCB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080845004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080845004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="28mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080845004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED0774R7M100DVCTCB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_865080845005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080845005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="35mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080845005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077100M100DVCTCB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_865081745005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081745005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="8uA"/>
<attribute name="I-RIPPLE" value="35mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081745005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077100M080DVCTCB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
<technology name="_865081745006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081745006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="17600uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081745006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077220M080DVCTCB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_8X6.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_8X6.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080149011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080149011.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="290mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080149011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE065331M6R3DVCTBB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080249010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080249010.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="285mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080249010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE065221M010DVCTBB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080349011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080349011.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080349011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE065151M016DVCTBB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080349013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080349013.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="285mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080349013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE065221M016DVCTBB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080449011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080449011.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080449011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE065101M025DVCTBB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080649011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080649011.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080649011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE065330M050DVCTBB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080649013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080649013.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080649013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE065470M050DVCTBB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_8X10.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_8X10.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080153012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080153012.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="450mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080153012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105471M6R3DVCTEB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080153013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080153013.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="42.84uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080153013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105681M6R3DVCTEB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080153014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080153014.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="530mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080153014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105102M6R3DVCTEB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080253011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080253011.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080253011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105331M010DVCTEB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080253012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080253012.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080253012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105471M010DVCTEB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080353014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080353014.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080353014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105331M016DVCTEB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080353015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080353015.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="590mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080353015 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105471M016DVCTEB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080453012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080453012.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080453012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105151M025DVCTEB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080453013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080453013.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="530mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080453013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105221M025DVCTEB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080453014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080453014.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="570mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080453014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105331M025DVCTEB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080553013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080553013.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="510mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080553013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105151M035DVCTEB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080553014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080553014.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="570mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080553014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105221M035DVCTEB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080653014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080653014.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="28uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080653014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105560M050DVCTEB000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080653015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080653015.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="320mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080653015 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105680M050DVCTEB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080653016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080653016.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080653016 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105101M050DVCTEB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080753012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080753012.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="112mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080753012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105330M063DVCTEB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080753013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080753013.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="119mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080753013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105470M063DVCTEB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080853006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080853006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080853006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105220M100DVCTEB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_865081753007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081753007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="26.4uA"/>
<attribute name="I-RIPPLE" value="112mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081753007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105330M080DVCTEB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_6.3X6.1" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_6.3X6.1(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080864003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080864003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="L" value="6.1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080864003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED0613R3M100DVCTBB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_10X10.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_10X10.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080157015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080157015.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080157015 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105122M6R3DVCTEB000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080157016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080157016.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="650mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080157016 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105152M6R3DVCTEB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080257013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080257013.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080257013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105681M010DVCTEB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080257014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080257014.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="740mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080257014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105102M010DVCTEB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080357016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080357016.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="720mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080357016 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105681M016DVCTEB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080457015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080457015.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="650mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080457015 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105471M025DVCTEB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080557015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080557015.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="650mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080557015 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105331M035DVCTEB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080657017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080657017.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080657017 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105151M050DVCTEB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080657018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080657018.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="650mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080657018 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105221M050DVCTEB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080757014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080757014.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080757014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105101M063DVCTEB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080857007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080857007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="135mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080857007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105330M100DVCTEB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_865081757008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081757008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="37.6uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081757008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105470M080DVCTEB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLI_5X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14723v209%20Family_WCAP-ASLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLI_5X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865080142005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080142005.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.53uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080142005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055560M6R3DVCTBB000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080142006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080142006.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.28uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080142006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055680M6R3DVCTBB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080142007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080142007.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080142007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055101M6R3DVCTBB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865080242002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080242002.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080242002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055270M010DVCTBB000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080242004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080242004.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="165mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080242004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055470M010DVCTBB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865080342004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080342004.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.32uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080342004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055270M016DVCTBB000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080342006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080342006.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="195mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080342006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055470M016DVCTBB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865080442003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080442003.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.75uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080442003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055150M025DVCTBB000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080442004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080442004.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="145mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080442004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055220M025DVCTBB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080442006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080442006.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080442006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055330M025DVCTBB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865080542005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080542005.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.25uA"/>
<attribute name="I-RIPPLE" value="140mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080542005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055150M035DVCTBB000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080542006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080542006.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="155mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080542006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055220M035DVCTBB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865080642005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080642005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.4uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080642005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC0556R8M050DVCTBB000"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080642006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080642006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="95mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080642006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055100M050DVCTBB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865080742008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080742008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="14mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080742008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC0553R3M063DVCTBB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865080742009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865080742009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="22mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865080742009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC0554R7M063DVCTBB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_865081742002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865081742002.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="12mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865081742002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC0552R2M080DVCTBB000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
