<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ASLU&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-03&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ASLU_5X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X5.5X1.4(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLU_3X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,3X5.5X0.8(DiameterXLengthXPitch)</description>
</package>
<package name="WCAP-ASLU_4X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,4X5.5X1(DiameterXLengthXPitch)</description>
</package>
<package name="WCAP-ASLU_6.3X7.7(DXL)">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X7.7X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLU_8X6.5(DXL)">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X6.5X2.3(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLU_6.3X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X5.5X2.1(DiameterXLengthXP)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ASLU_5X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 330 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 1000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 3.0 x 5.5 up to 8.0 x 6.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLU/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLU/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_5X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090142005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090142005.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="1.26uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090142005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBC055101M6R3DVCTBA000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.948027Ohm"/>
</technology>
<technology name="_865090242003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090242003.pdf"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="0.66uA"/>
<attribute name="I-RIPPLE" value="41mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090242003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBC055330M010DVCTBA000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="1.52562Ohm"/>
</technology>
<technology name="_865090342003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090342003.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="0.704uA"/>
<attribute name="I-RIPPLE" value="37mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090342003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBC055220M016DVCTBA000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="1.78245Ohm"/>
</technology>
<technology name="_865090442004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090442004.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="1.1uA"/>
<attribute name="I-RIPPLE" value="42mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090442004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBC055220M025DVCTBA000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="1.83969Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_4X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 330 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 1000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 3.0 x 5.5 up to 8.0 x 6.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLU/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLU/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_4X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090140001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090140001.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="15mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090140001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055100M6R3DVCTAA000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="2.47788Ohm"/>
</technology>
<technology name="_865090140002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090140002.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="28mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090140002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055220M6R3DVCTAA000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="2.30648Ohm"/>
</technology>
<technology name="_865090140003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090140003.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4158uA"/>
<attribute name="I-RIPPLE" value="37mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090140003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055330M6R3DVCTAA000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="1.88263Ohm"/>
</technology>
<technology name="_865090140004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090140004.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.5922uA"/>
<attribute name="I-RIPPLE" value="45mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090140004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055470M6R3DVCTAA000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="2.62971Ohm"/>
</technology>
<technology name="_865090240001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090240001.pdf"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="23mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090240001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055100M010DVCTAA000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="2.89456Ohm"/>
</technology>
<technology name="_865090240002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090240002.pdf"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.44uA"/>
<attribute name="I-RIPPLE" value="33mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090240002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055220M010DVCTAA000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="3.38993Ohm"/>
</technology>
<technology name="_865090340001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090340001.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="10mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090340001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0554R7M016DVCTAA000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="3.54301Ohm"/>
</technology>
<technology name="_865090340002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090340002.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="23mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090340002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055100M016DVCTAA000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="2.35078Ohm"/>
</technology>
<technology name="_865090440001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090440001.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="10mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090440001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0553R3M025DVCTAA000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="3.14324Ohm"/>
</technology>
<technology name="_865090440002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090440002.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="16mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090440002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0554R7M025DVCTAA000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="3.663Ohm"/>
</technology>
<technology name="_865090440003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090440003.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="27mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090440003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055100M025DVCTAA000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="2.29162Ohm"/>
</technology>
<technology name="_865090540001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090540001.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="8.4mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090540001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0552R2M035DVCTAA000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="3.63846Ohm"/>
</technology>
<technology name="_865090540002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090540002.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="15mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090540002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0553R3M035DVCTAA000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="3.23821Ohm"/>
</technology>
<technology name="_865090540003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090540003.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="18mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090540003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0554R7M035DVCTAA000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="3.57419Ohm"/>
</technology>
<technology name="_865090640001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090640001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="1mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090640001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055R10M050DVCTAA000"/>
<attribute name="VALUE" value="0.1  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="31.5098Ohm"/>
</technology>
<technology name="_865090640002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090640002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="2mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090640002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055R22M050DVCTAA000"/>
<attribute name="VALUE" value="0.22  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="17.494Ohm"/>
</technology>
<technology name="_865090640003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090640003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="2.8mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090640003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055R33M050DVCTAA000"/>
<attribute name="VALUE" value="0.33  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="14.0887Ohm"/>
</technology>
<technology name="_865090640004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090640004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="4mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090640004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055R47M050DVCTAA000"/>
<attribute name="VALUE" value="0.47  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="12.9225Ohm"/>
</technology>
<technology name="_865090640005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090640005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="8.4mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090640005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055010M050DVCTAA000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="4.74567Ohm"/>
</technology>
<technology name="_865090640006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090640006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="13mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090640006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0552R2M050DVCTAA000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090640007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090640007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090640007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0553R3M050DVCTAA000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="3.1572Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_3X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 330 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 1000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 3.0 x 5.5 up to 8.0 x 6.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLU/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLU/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_3X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090168010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090168010.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="25mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090168010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055220M6R3DVCTAB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090268009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090268009.pdf"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="18mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090268009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055100M010DVCTAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090368008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090368008.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090368008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055100M016DVCTAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090468010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090468010.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="11mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090468010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA0553R3M025DVCTAB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090468011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090468011.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="15mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090468011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA0554R7M025DVCTAB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090668014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090668014.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="1mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090668014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055R10M050DVCTAB000"/>
<attribute name="VALUE" value="0.1  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090668015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090668015.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="2mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090668015 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055R22M050DVCTAB000"/>
<attribute name="VALUE" value="0.22  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090668016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090668016.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="2mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090668016 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055R33M050DVCTAB000"/>
<attribute name="VALUE" value="0.33  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090768002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090768002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="1mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090768002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055R10M063DVCTAB000"/>
<attribute name="VALUE" value="0.1  µF "/>
<attribute name="VR" value="63V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090768003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090768003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="2mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090768003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055R22M063DVCTAB000"/>
<attribute name="VALUE" value="0.22  µF "/>
<attribute name="VR" value="63V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090768004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090768004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="2mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090768004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055R33M063DVCTAB000"/>
<attribute name="VALUE" value="0.33  µF "/>
<attribute name="VR" value="63V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090768005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090768005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="3mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090768005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBA055R47M063DVCTAB000"/>
<attribute name="VALUE" value="0.47  µF "/>
<attribute name="VR" value="63V(DC)"/>
<attribute name="Z" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_6.3X7.7" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 330 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 1000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 3.0 x 5.5 up to 8.0 x 6.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLU/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLU/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_6.3X7.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090145006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090145006.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="2.772uA"/>
<attribute name="I-RIPPLE" value="102mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090145006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077221M6R3DVCTCA000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090145008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090145008.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="4.158uA"/>
<attribute name="I-RIPPLE" value="155mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090145008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077331M6R3DVCTCA000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.299847Ohm"/>
</technology>
<technology name="_865090245005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090245005.pdf"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="2uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090245005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077101M010DVCTCA000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.373722Ohm"/>
</technology>
<technology name="_865090245007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090245007.pdf"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="4.4uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090245007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077221M010DVCTCA000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.312683Ohm"/>
</technology>
<technology name="_865090345006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090345006.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3.2uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090345006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077101M016DVCTCA000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="0.366329Ohm"/>
</technology>
<technology name="_865090445006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090445006.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="2.35uA"/>
<attribute name="I-RIPPLE" value="65mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090445006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077470M025DVCTCA000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="0.589952Ohm"/>
</technology>
<technology name="_865090445008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090445008.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="102mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090445008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077101M025DVCTCA000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="0.547075Ohm"/>
</technology>
<technology name="_865090545006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090545006.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="2.31uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090545006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077330M035DVCTCA000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="0.62377Ohm"/>
</technology>
<technology name="_865090545008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090545008.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3.29uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090545008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077470M035DVCTCA000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="0.585673Ohm"/>
</technology>
<technology name="_865090645010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090645010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="2.2uA"/>
<attribute name="I-RIPPLE" value="48mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090645010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077220M050DVCTCA000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="0.698968Ohm"/>
</technology>
<technology name="_865090645012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090645012.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="66mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090645012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077330M050DVCTCA000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="0.598977Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_8X6.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 330 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 1000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 3.0 x 5.5 up to 8.0 x 6.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLU/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLU/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_8X6.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090149007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090149007.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="2.772uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090149007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065221M6R3DVCTBA000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.392113Ohm"/>
</technology>
<technology name="_865090149009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090149009.pdf"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="4.158uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090149009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065331M6R3DVCTBA000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.402681Ohm"/>
</technology>
<technology name="_865090249006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090249006.pdf"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="2uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090249006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065101M010DVCTBA000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.486738Ohm"/>
</technology>
<technology name="_865090249008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090249008.pdf"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="4.4uA"/>
<attribute name="I-RIPPLE" value="135mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090249008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065221M010DVCTBA000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.413975Ohm"/>
</technology>
<technology name="_865090349007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090349007.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="3.2uA"/>
<attribute name="I-RIPPLE" value="92mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090349007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065101M016DVCTBA000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="0.411992Ohm"/>
</technology>
<technology name="_865090449007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090449007.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="2.35uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090449007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065470M025DVCTBA000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="0.614421Ohm"/>
</technology>
<technology name="_865090449009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090449009.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090449009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065101M025DVCTBA000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090549007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090549007.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="2.31uA"/>
<attribute name="I-RIPPLE" value="62mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090549007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065330M035DVCTBA000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="0.591377Ohm"/>
</technology>
<technology name="_865090549009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090549009.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="3.29uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090549009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065470M035DVCTBA000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="0.659394Ohm"/>
</technology>
<technology name="_865090649011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090649011.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="2.2uA"/>
<attribute name="I-RIPPLE" value="52mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090649011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065220M050DVCTBA000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="0.689357Ohm"/>
</technology>
<technology name="_865090649013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090649013.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="71mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090649013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065330M050DVCTBA000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="0.602919Ohm"/>
</technology>
<technology name="_865090749001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090749001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="14uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090749001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065220M063DVCTBB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value=""/>
<attribute name="Z" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_6.3X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 330 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 1000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 3.0 x 5.5 up to 8.0 x 6.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14725v209%20Family_WCAP-ASLU.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASLU/"&gt;https://www.we-online.com/catalog/en/WCAP-ASLU/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_6.3X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090243004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090243004.pdf"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="0.94uA"/>
<attribute name="I-RIPPLE" value="52mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090243004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055470M010DVCTBA000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.881982Ohm"/>
</technology>
<technology name="_865090343004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090343004.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="1.056uA"/>
<attribute name="I-RIPPLE" value="49mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090343004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055330M016DVCTBA000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="0.762218Ohm"/>
</technology>
<technology name="_865090343005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090343005.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="1.504uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090343005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055470M016DVCTBA000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="1.40507Ohm"/>
</technology>
<technology name="_865090443005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090443005.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="1.65uA"/>
<attribute name="I-RIPPLE" value="52mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090443005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055330M025DVCTBA000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="1.02509Ohm"/>
</technology>
<technology name="_865090543004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090543004.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="0.7uA"/>
<attribute name="I-RIPPLE" value="29mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090543004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055100M035DVCTBA000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="0.872475Ohm"/>
</technology>
<technology name="_865090543005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090543005.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="1.54uA"/>
<attribute name="I-RIPPLE" value="46mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090543005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055220M035DVCTBA000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="1.84559Ohm"/>
</technology>
<technology name="_865090643008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090643008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="0.47uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090643008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD0554R7M050DVCTBA000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865090643009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865090643009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="1uA"/>
<attribute name="I-RIPPLE" value="33mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865090643009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055100M050DVCTBA000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="2.84992Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
