<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - ESD Protection - WE-VE femtoF&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-10-07&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-VE_FEMTOF_0603">
<description>&lt;b&gt;WE-VE femtoF ESD Suppressor
&lt;br&gt;&lt;/b&gt;Size  : 0603
&lt;br&gt;L X W X H = 1.6mm X 0.8mm X 0.9mm</description>
</package>
<package name="WE-VE_FEMTOF_0402">
<description>&lt;b&gt;WE-VE femtoF ESD Suppressor
&lt;br&gt;&lt;/b&gt;Size  : 0402
&lt;br&gt;L X W X H = 1mm X 0.5mm X 0.6mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-VE_FEMTOF">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-VE_FEMTOF_0603" prefix="D">
<description>&lt;b&gt; WE-VE femtoF ESD Suppressor

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Lowest Capacitance
&lt;br&gt;Fast response time
&lt;br&gt;Low leakage current
&lt;br&gt;Low clamping voltage
&lt;br&gt;Almost no energy consumption in stand-by mode
&lt;br&gt;Excellent absorption for ESD-impulses
&lt;br&gt;Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;Nickel barrier


&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Protection of, data lines, bus systems or semiconductors
&lt;br&gt;ESD protection in accordance with EN 61000-4-2: 
&lt;br&gt; 8 kV contact discharge 
 &lt;br&gt;15 kV air discharge

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o157489v209%20Family_WE-VE_femtoF_0402_0603.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o157489v209%20Family_WE-VE_femtoF_0402_0603.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-VE_FEMTOF"&gt;https://katalog.we-online.de/en/pbs/WE-VE_FEMTOF&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-09&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VE_FEMTOF"/>
</gates>
<devices>
<device name="" package="WE-VE_FEMTOF_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8231606A">
<attribute name="CCH-TYP" value="0.05pF"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/8231606A.pdf"/>
<attribute name="ILEAK" value="0.05uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="8231606A"/>
<attribute name="VALUE" value="6V"/>
<attribute name="VCH-TYP" value="40V"/>
<attribute name="VESD-AIR" value="15kV"/>
<attribute name="VESD-CONTACT" value="8kV"/>
</technology>
<technology name="_8231614A">
<attribute name="CCH-TYP" value="0.05pF"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/8231614A.pdf"/>
<attribute name="ILEAK" value="0.05uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="8231614A"/>
<attribute name="VALUE" value="14V"/>
<attribute name="VCH-TYP" value="45V"/>
<attribute name="VESD-AIR" value="15kV"/>
<attribute name="VESD-CONTACT" value="8kV"/>
</technology>
<technology name="_8231626A">
<attribute name="CCH-TYP" value="0.05pF"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/8231626A.pdf"/>
<attribute name="ILEAK" value="0.05uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="8231626A"/>
<attribute name="VALUE" value="26V"/>
<attribute name="VCH-TYP" value="50V"/>
<attribute name="VESD-AIR" value="15kV"/>
<attribute name="VESD-CONTACT" value="8kV"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VE_FEMTOF_0402" prefix="D">
<description>&lt;b&gt; WE-VE femtoF ESD Suppressor

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Lowest Capacitance
&lt;br&gt;Fast response time
&lt;br&gt;Low leakage current
&lt;br&gt;Low clamping voltage
&lt;br&gt;Almost no energy consumption in stand-by mode
&lt;br&gt;Excellent absorption for ESD-impulses
&lt;br&gt;Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;Nickel barrier


&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Protection of, data lines, bus systems or semiconductors
&lt;br&gt;ESD protection in accordance with EN 61000-4-2: 
&lt;br&gt; 8 kV contact discharge 
 &lt;br&gt;15 kV air discharge

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o157489v209%20Family_WE-VE_femtoF_0402_0603.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o157489v209%20Family_WE-VE_femtoF_0402_0603.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-VE_FEMTOF"&gt;https://katalog.we-online.de/en/pbs/WE-VE_FEMTOF&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-09&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VE_FEMTOF"/>
</gates>
<devices>
<device name="" package="WE-VE_FEMTOF_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8231706A">
<attribute name="CCH-TYP" value="0.05pF"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/8231706A.pdf"/>
<attribute name="ILEAK" value="0.05uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="8231706A"/>
<attribute name="VALUE" value="6V"/>
<attribute name="VCH-TYP" value="40V"/>
<attribute name="VESD-AIR" value="15kV"/>
<attribute name="VESD-CONTACT" value="8kV"/>
</technology>
<technology name="_8231714A">
<attribute name="CCH-TYP" value="0.05pF"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/8231714A.pdf"/>
<attribute name="ILEAK" value="0.05uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="8231714A"/>
<attribute name="VALUE" value="14V"/>
<attribute name="VCH-TYP" value="45V"/>
<attribute name="VESD-AIR" value="15kV"/>
<attribute name="VESD-CONTACT" value="8kV"/>
</technology>
<technology name="_8231726A">
<attribute name="CCH-TYP" value="0.5pF"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/8231726A.pdf"/>
<attribute name="ILEAK" value="0.05uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="8231726A"/>
<attribute name="VALUE" value="26V"/>
<attribute name="VCH-TYP" value="50V"/>
<attribute name="VESD-AIR" value="15kV"/>
<attribute name="VESD-CONTACT" value="8kV"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
