<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - DC Power Jacks - WR-DC &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-09-30&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="694102303002">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (4.2)</description>
</package>
<package name="694108105102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled SMT Ø 6.4 with pegs</description>
</package>
<package name="694108402002">
<description>&lt;b&gt;WR-DC DC Power Jack Vertical THT Ø 6.4</description>
</package>
<package name="694103107102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled Low Profile SMT Ø 3.9 with 4 soldering pads &amp; pegs</description>
</package>
<package name="694102304002">
<description>&lt;b&gt;WR-DC DC Power Jack THT Right Angled Low Profile (3.8)</description>
</package>
<package name="694108301002">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (6.4)</description>
</package>
<package name="694106402002">
<description>&lt;b&gt;WR-DC DC Power Jack Vertical THT Ø 6.4</description>
</package>
<package name="694102107102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled Low Profile SMT Ø 3.9 with 4 soldering pads &amp; pegs</description>
</package>
<package name="694103304002">
<description>&lt;b&gt;WR-DC DC Power Jack THT Right Angled Low Profile (3.8)</description>
</package>
<package name="694105309102">
<description>&lt;b&gt;WR-DC Power Jack Right Angled Shielded THT Ø 4.93</description>
</package>
<package name="694106106102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled SMT Ø 6.4 with 4 soldering pads &amp; pegs</description>
</package>
<package name="694106301002">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (6.4)</description>
</package>
<package name="694106105102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled SMT Ø 6.4 with pegs</description>
</package>
<package name="694103303002">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (4.2)</description>
</package>
<package name="694101308002">
<description>&lt;b&gt;WR-DC DC Power Jack THT Right Angled Low Profile (2.8)</description>
</package>
<package name="694106210102">
<description>&lt;b&gt;WR-DC DC Power Jack Vertical SMT Ø 2.0 &amp; Ø 2.5</description>
</package>
<package name="694108106102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled SMT Ø 6.4 with 4 soldering pads &amp; pegs</description>
</package>
<package name="694108210102">
<description>&lt;b&gt;WR-DC DC Power Jack Vertical SMT Ø 2.0 &amp; Ø 2.5</description>
</package>
</packages>
<symbols>
<symbol name="WR-DC">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="694102303002" prefix="J">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (4.2)
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 2 A 
&lt;br&gt;Working Voltage 30 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Bag 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64601v209%20Family_WR-DC_THT_6941xx303002.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64601v209%20Family_WR-DC_THT_6941xx303002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_RIGHT_ANGLED_4_2_69410X303002"&gt;https://www.we-online.com/catalog/en/DC_RIGHT_ANGLED_4_2_69410X303002&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694102303002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694102303002.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694102303002 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694102303002 "/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694108105102" prefix="J">
<description>&lt;b&gt; WR-DC DC Power Jack Right Angled SMT Ø 6.4 with pegs
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material Plastic 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 5 A 
&lt;br&gt;Working Voltage 24 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58992v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_SMT_694106105102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58992v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_SMT_694106105102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_6_4_WITH_PEGS_69410X105102"&gt;https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_6_4_WITH_PEGS_69410X105102&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-01&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694108105102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694108105102.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 694108105102 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694108105102 "/>
<attribute name="WORKING-VOLTAGE" value="24V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694108402002" prefix="J">
<description>&lt;b&gt; WR-DC DC Power Jack Vertical THT Ø 6.4
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Vertical 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 3 A 
&lt;br&gt;Working Voltage 20 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Bag 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64599v209%20Family_WR-DC_THT_6941xx402002_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64599v209%20Family_WR-DC_THT_6941xx402002_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_THT_VERTICAL_6_4_69410X402002"&gt;https://www.we-online.com/catalog/en/DC_THT_VERTICAL_6_4_69410X402002&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694108402002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694108402002.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694108402002 "/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 694108402002 "/>
<attribute name="WORKING-VOLTAGE" value="20V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694103107102" prefix="J">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled Low Profile SMT Ø 3.9 with 4 soldering pads &amp; pegs
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 5 A 
&lt;br&gt;Working Voltage 18 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o59004v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_Low_SMT_694102107102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o59004v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_Low_SMT_694102107102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_LOW_PROFILE_3_9_WITH_4_SOLDER_PADS_PEGS_69410X107102"&gt;https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_LOW_PROFILE_3_9_WITH_4_SOLDER_PADS_PEGS_69410X107102&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-01&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694103107102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694103107102.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 694103107102 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694103107102 "/>
<attribute name="WORKING-VOLTAGE" value="18V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694102304002" prefix="J">
<description>&lt;b&gt;WR-DC DC Power Jack THT Right Angled Low Profile (3.8)
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Tip Spring Plating Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 24 V (DC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 30 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60887v209%20Family_Con_WR-DC_THT_6941xx304002_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60887v209%20Family_Con_WR-DC_THT_6941xx304002_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_THT_RIGHT_ANGLED_LOW_PROFILE_3_8_69410X304002"&gt;https://www.we-online.com/catalog/en/DC_THT_RIGHT_ANGLED_LOW_PROFILE_3_8_69410X304002&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694102304002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694102304002.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694102304002 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694102304002 "/>
<attribute name="WORKING-VOLTAGE" value="24V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694108301002" prefix="J">
<description>&lt;b&gt; WR-DC DC Power Jack Right Angled (6.4)
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 5 A 
&lt;br&gt;Working Voltage 30 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Bag 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o59009v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_THT_69410x301002.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o59009v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_THT_69410x301002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_RIGHT_ANGLED_6_4_69410X301002"&gt;https://www.we-online.com/catalog/en/DC_RIGHT_ANGLED_6_4_69410X301002&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694108301002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694108301002.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694108301002 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694108301002 "/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694106402002" prefix="J">
<description>&lt;b&gt; WR-DC DC Power Jack Vertical THT Ø 6.4
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Vertical 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 3 A 
&lt;br&gt;Working Voltage 20 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Bag 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64599v209%20Family_WR-DC_THT_6941xx402002_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64599v209%20Family_WR-DC_THT_6941xx402002_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_THT_VERTICAL_6_4_69410X402002"&gt;https://www.we-online.com/catalog/en/DC_THT_VERTICAL_6_4_69410X402002&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694106402002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694106402002.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694106402002 "/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 694106402002 "/>
<attribute name="WORKING-VOLTAGE" value="20V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694103304002" prefix="J">
<description>&lt;b&gt;WR-DC DC Power Jack THT Right Angled Low Profile (3.8)
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Tip Spring Plating Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 24 V (DC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 30 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60887v209%20Family_Con_WR-DC_THT_6941xx304002_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60887v209%20Family_Con_WR-DC_THT_6941xx304002_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_THT_RIGHT_ANGLED_LOW_PROFILE_3_8_69410X304002"&gt;https://www.we-online.com/catalog/en/DC_THT_RIGHT_ANGLED_LOW_PROFILE_3_8_69410X304002&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694103304002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694103304002.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694103304002 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694103304002 "/>
<attribute name="WORKING-VOLTAGE" value="24V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694102107102" prefix="J">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled Low Profile SMT Ø 3.9 with 4 soldering pads &amp; pegs
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 5 A 
&lt;br&gt;Working Voltage 18 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o59004v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_Low_SMT_694102107102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o59004v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_Low_SMT_694102107102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_LOW_PROFILE_3_9_WITH_4_SOLDER_PADS_PEGS_69410X107102"&gt;https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_LOW_PROFILE_3_9_WITH_4_SOLDER_PADS_PEGS_69410X107102&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-01&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694102107102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694102107102.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 694102107102 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694102107102 "/>
<attribute name="WORKING-VOLTAGE" value="18V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694105309102" prefix="J">
<description>&lt;b&gt;WR-DC Power Jack Right Angled Shielded THT Ø 4.93
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material Brass 
&lt;br&gt;Shielding Plating Nickel 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 5.5 A 
&lt;br&gt;Working Voltage 20 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 30 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60613v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_THT_694105309102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60613v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_THT_694105309102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_THT_RIGHT_ANGLED_SHIELDED_4_93_694105309102"&gt;https://www.we-online.com/catalog/en/DC_THT_RIGHT_ANGLED_SHIELDED_4_93_694105309102&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694105309102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694105309102.pdf"/>
<attribute name="IR" value="5.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694105309102 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694105309102 "/>
<attribute name="WORKING-VOLTAGE" value="20V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694106106102" prefix="J">
<description>&lt;b&gt; WR-DC DC Power Jack Right Angled SMT Ø 6.4 with 4 soldering pads &amp; pegs
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;
&lt;/b&gt;IR 1 5 A 
&lt;br&gt;Working Voltage 24 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58999v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_SMT_694108106102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58999v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_SMT_694108106102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_6_4_WITH_4_SOLDER_PADS_PEGS_69410X106102"&gt;https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_6_4_WITH_4_SOLDER_PADS_PEGS_69410X106102&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-01&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694106106102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694106106102.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 694106106102 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694106106102 "/>
<attribute name="WORKING-VOLTAGE" value="24V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694106105102" prefix="J">
<description>&lt;b&gt; WR-DC DC Power Jack Right Angled SMT Ø 6.4 with pegs
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material Plastic 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 5 A 
&lt;br&gt;Working Voltage 24 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58992v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_SMT_694106105102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58992v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_SMT_694106105102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_6_4_WITH_PEGS_69410X105102"&gt;https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_6_4_WITH_PEGS_69410X105102&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-01&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694106105102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694106105102.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 694106105102 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694106105102 "/>
<attribute name="WORKING-VOLTAGE" value="24V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694106301002" prefix="J">
<description>&lt;b&gt; WR-DC DC Power Jack Right Angled (6.4)
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 5 A 
&lt;br&gt;Working Voltage 30 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Bag 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o59009v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_THT_69410x301002.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o59009v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_THT_69410x301002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_RIGHT_ANGLED_6_4_69410X301002"&gt;https://www.we-online.com/catalog/en/DC_RIGHT_ANGLED_6_4_69410X301002&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694106301002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694106301002.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694106301002 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694106301002 "/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694103303002" prefix="J">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (4.2)
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 2 A 
&lt;br&gt;Working Voltage 30 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Bag 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64601v209%20Family_WR-DC_THT_6941xx303002.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64601v209%20Family_WR-DC_THT_6941xx303002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_RIGHT_ANGLED_4_2_69410X303002"&gt;https://www.we-online.com/catalog/en/DC_RIGHT_ANGLED_4_2_69410X303002&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694103303002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694103303002.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694103303002 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694103303002 "/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694101308002" prefix="J">
<description>&lt;b&gt;WR-DC DC Power Jack THT Right Angled Low Profile (2.8)
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 2 A 
&lt;br&gt;Working Voltage 12 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 30 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Bag 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60624v209%20Family_WR-DC_THT_694101308002_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60624v209%20Family_WR-DC_THT_694101308002_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DC_THT_RIGHT_ANGLED_LOW_PROFILE_2_8_694101308002"&gt;https://www.we-online.com/catalog/en/DC_THT_RIGHT_ANGLED_LOW_PROFILE_2_8_694101308002&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-09-30&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694101308002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694101308002.pdf"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 694101308002 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694101308002 "/>
<attribute name="WORKING-VOLTAGE" value="12V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694106210102" prefix="J">
<description>&lt;b&gt;WR-DC DC Power Jack Vertical SMT Ø 2.0 &amp; Ø 2.5
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Vertical 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA 9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold over Nickel 
&lt;br&gt;Center Pin Terminal Plating Tin over Nickel 
&lt;br&gt;Tip Spring Plating Tin over Nickel 
&lt;br&gt;Shunt Terminal Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 3.5 A 
&lt;br&gt;Working Voltage 30 V (DC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 30 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel &amp; Mylar 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o79412v209%20WR-DC_6941xx210102_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o79412v209%20WR-DC_6941xx210102_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/DC_SMT_VERTICAL_2_0-2_5_6941XX210102"&gt;https://katalog.we-online.com/en/em/DC_SMT_VERTICAL_2_0-2_5_6941XX210102&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-01&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694106210102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694106210102.pdf"/>
<attribute name="IR" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 694106210102 "/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 694106210102 "/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694108106102" prefix="J">
<description>&lt;b&gt; WR-DC DC Power Jack Right Angled SMT Ø 6.4 with 4 soldering pads &amp; pegs
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Right Angled 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold 
&lt;br&gt;Center Pin Terminal Plating Tin 
&lt;br&gt;Tip Spring Material Tin 
&lt;br&gt;Shunt Terminal Plating Tin 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;
&lt;/b&gt;IR 1 5 A 
&lt;br&gt;Working Voltage 24 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58999v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_SMT_694108106102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58999v209%20Family_WR-DC_DC_Power_Jack_Right_Angled_SMT_694108106102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_6_4_WITH_4_SOLDER_PADS_PEGS_69410X106102"&gt;https://katalog.we-online.com/en/em/DC_SMT_RIGHT_ANGLED_6_4_WITH_4_SOLDER_PADS_PEGS_69410X106102&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-01&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694108106102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694108106102.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 694108106102 "/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 694108106102 "/>
<attribute name="WORKING-VOLTAGE" value="24V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694108210102" prefix="D">
<description>&lt;b&gt;WR-DC DC Power Jack Vertical SMT Ø 2.0 &amp; Ø 2.5
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles 
&lt;br&gt;Type Vertical 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA 9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Center Pin Plating Gold over Nickel 
&lt;br&gt;Center Pin Terminal Plating Tin over Nickel 
&lt;br&gt;Tip Spring Plating Tin over Nickel 
&lt;br&gt;Shunt Terminal Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1 3.5 A 
&lt;br&gt;Working Voltage 30 V (DC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 30 mΩ 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel &amp; Mylar 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o79412v209%20WR-DC_6941xx210102_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o79412v209%20WR-DC_6941xx210102_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/DC_SMT_VERTICAL_2_0-2_5_6941XX210102"&gt;https://katalog.we-online.com/en/em/DC_SMT_VERTICAL_2_0-2_5_6941XX210102&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-01&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694108210102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/694108210102.pdf"/>
<attribute name="IR" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 694108210102 "/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 694108210102 "/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
