<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Resistors - Metal Plate Resistors - WRIS-PSMB&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Eagle Version 9, Library Revision 2019a, 2019-09-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WRIS-PSMB_0805_2.0X1.25X0.22X0.47(LXWXHXPW)">
</package>
<package name="WRIS-PSMB_2512_6.3X3.1X0.35X1.4(LXWXHXPW)">
</package>
<package name="WRIS-PSMB_0805_2.0X1.25X0.22X0.6(LXWXHXPW)">
</package>
<package name="WRIS-PSMB_0603_1.6X0.8X0.3X0.3(LXWXHXPW)">
<description>Hight= 0.3mm</description>
</package>
<package name="WRIS-PSMB_0603_1.6X0.8X0.35X0.6(LXWXHXPW)">
<description>Hight= 0.35mm</description>
</package>
</packages>
<symbols>
<symbol name="R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WRIS-PSMB_2512" prefix="R">
<description>&lt;b&gt; WRIS-PSMB Metal Plate Resistors
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Metal plate resistors
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55 °C up to +155 °C
&lt;br&gt;Resistance range: 5 mΩ up to 10 mΩ
&lt;br&gt;Resistance tolerance: ±1 %
&lt;br&gt;Rated power: 0.33 W up to 1 W
&lt;br&gt;Enhanced current sensing
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DMotor control
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;L X W X H X PW =Length X Width X Height X Pad Width
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135743v209%20Family_WRIS-PSMB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135743v209%20Family_WRIS-PSMB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-PSMB"&gt;https://katalog.we-online.com/en/pbs/WRIS-PSMB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun, Shan 2018-11-14&lt;br&gt;
&lt;/b&gt;2018(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_6.3X3.1X0.35X1.4" package="WRIS-PSMB_2512_6.3X3.1X0.35X1.4(LXWXHXPW)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060763005">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/580060763005.pdf"/>
<attribute name="IR" value="12A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 580060763005 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="MB2512R007F101KAATE0000"/>
<attribute name="VALUE" value="7mOhm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-PSMB_0805" prefix="R">
<description>&lt;b&gt; WRIS-PSMB Metal Plate Resistors
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Metal plate resistors
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55 °C up to +155 °C
&lt;br&gt;Resistance range: 5 mΩ up to 10 mΩ
&lt;br&gt;Resistance tolerance: ±1 %
&lt;br&gt;Rated power: 0.33 W up to 1 W
&lt;br&gt;Enhanced current sensing
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DMotor control
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;L X W X H X PW =Length X Width X Height X Pad Width
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135743v209%20Family_WRIS-PSMB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135743v209%20Family_WRIS-PSMB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-PSMB"&gt;https://katalog.we-online.com/en/pbs/WRIS-PSMB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun, Shan 2018-11-14&lt;br&gt;
&lt;/b&gt;2018(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_2.0X1.25X0.22X0.47" package="WRIS-PSMB_0805_2.0X1.25X0.22X0.47(LXWXHXPW)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060720008">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/580060720008.pdf"/>
<attribute name="IR" value="7.07A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 580060720008 "/>
<attribute name="PRATED" value="0.5W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="MB0805R010F102KAATP0000"/>
<attribute name="VALUE" value="10mOhm"/>
</technology>
</technologies>
</device>
<device name="_2.0X1.25X0.22X0.6" package="WRIS-PSMB_0805_2.0X1.25X0.22X0.6(LXWXHXPW)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060720003">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/580060720003.pdf"/>
<attribute name="IR" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 580060720003 "/>
<attribute name="PRATED" value="0.5W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="MB0805R005F102KAATP0000"/>
<attribute name="VALUE" value="5mOhm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-PSMB_0603" prefix="R">
<description>&lt;b&gt; WRIS-PSMB Metal Plate Resistors
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Metal plate resistors
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55 °C up to +155 °C
&lt;br&gt;Resistance range: 5 mΩ up to 10 mΩ
&lt;br&gt;Resistance tolerance: ±1 %
&lt;br&gt;Rated power: 0.33 W up to 1 W
&lt;br&gt;Enhanced current sensing
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DMotor control
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;L X W X H X PW =Length X Width X Height X Pad Width
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135743v209%20Family_WRIS-PSMB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135743v209%20Family_WRIS-PSMB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-PSMB"&gt;https://katalog.we-online.com/en/pbs/WRIS-PSMB&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun, Shan 2018-11-14&lt;br&gt;
&lt;/b&gt;2018(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_1.6X0.8X0.3X0.3" package="WRIS-PSMB_0603_1.6X0.8X0.3X0.3(LXWXHXPW)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060716002">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/580060716002.pdf"/>
<attribute name="IR" value="5.74A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 580060716002 "/>
<attribute name="PRATED" value="0.33W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="MB0603R010F103KAATP0000"/>
<attribute name="VALUE" value="10mOhm"/>
</technology>
</technologies>
</device>
<device name="_1.6X0.8X0.35X0.6" package="WRIS-PSMB_0603_1.6X0.8X0.35X0.6(LXWXHXPW)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_580060716001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/580060716001.pdf"/>
<attribute name="IR" value="8.12A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 580060716001 "/>
<attribute name="PRATED" value="0.33W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="MB0603R005F103KAATP0000"/>
<attribute name="VALUE" value="5mOhm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
