<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Switches - Encoder Switches - WS-ENTV&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-05-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WS-ENTV_482024764004">
<description>&lt;b&gt;WS-ENTV Mechanical Incremental Encoder Switch 12.4x13.20mm Plastic Shaft without bushing
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;12.4x13.20mm</description>
</package>
<package name="WS-ENTV_4820XX714003">
<description>&lt;b&gt;WS-ENTV Mechanical Incremental Encoder Switch 12.4x13.20mm Plastic Shaft with Threaded bushing
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;12.4x13.20mm</description>
</package>
<package name="WS-ENTV_4820XX514001">
<description>&lt;B&gt;WS-ENTV Mechanical Incremental Encoder Switch 11.7x13.75mm Metal Shaft with bushing
&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;11.7x13.75mm</description>
</package>
<package name="WS-ENTV_482016564002">
<description>&lt;b&gt;WS-ENTV Mechanical Incremental Encoder Switch 11.7x12.00mm Metal Shaft with Plain bushing
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;11.7x12.00mm</description>
</package>
</packages>
<symbols>
<symbol name="WS-ENTV_482024764004">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="COM" direction="pas"/>
</symbol>
<symbol name="WS-ENTV_482012714003">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="WS-ENTV_482009514001">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="COM" direction="pas"/>
</symbol>
<symbol name="WS-ENTV_482016514001">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="COM" direction="pas"/>
</symbol>
<symbol name="WS-ENTV_482020514001">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="COM" direction="pas"/>
</symbol>
<symbol name="WS-ENTV_482016564002">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="482024764004" prefix="S">
<description>&lt;b&gt;WS-ENTV Mechanical Incremental Encoder Switch 12.4x13.20mm Plastic Shaft without bushing

&lt;br&gt;
&lt;br&gt;
Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	PC
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Actuator Color	Black
&lt;br&gt;Frame Material	PBT
&lt;br&gt;Frame Flammability Rating	UL94 HB
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Silver
&lt;br&gt;Frame Color	Black
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;Packaging Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;IR	10 mA
&lt;BR&gt;VR	5 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	300 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Electrical Life Encoder	30000 Cycles
&lt;BR&gt;Electrical Life Switch	20000 Cycles
&lt;BR&gt;Detent	24 Positions
&lt;BR&gt;Torque Encoder	20 mN*m
&lt;BR&gt;Operation Force (Value)	300 g
&lt;BR&gt;Travel	0.5 mm
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o343310v209%20Family_WS-ENTV_482024764004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o343310v209%20Family_WS-ENTV_482024764004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ENTV_MECHANICAL_INCREMENTAL_ENCODER_SWITCH_12_4_13_2_PLASTIC_SHAFT_WITHOUT_BUSHING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WS_ENTV_MECHANICAL_INCREMENTAL_ENCODER_SWITCH_12_4_13_2_PLASTIC_SHAFT_WITHOUT_BUSHING&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-05-29&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ENTV_482024764004"/>
</gates>
<devices>
<device name="" package="WS-ENTV_482024764004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="COM" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/482024764004?ae"/>
<attribute name="DETENT" value="24 Positions"/>
<attribute name="ELECTRICAL-LIFE-ENCODER" value="30000 Cycles"/>
<attribute name="ELECTRICAL-LIFE-SWITCH" value="20000 Cycles"/>
<attribute name="PART-NUMBER" value="482024764004"/>
<attribute name="RESOLUTION" value="24 Pulse/360 degree"/>
<attribute name="VALUE" value="482024764004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="482009514001" prefix="S">
<description>&lt;b&gt;WS-ENTV Mechanical Incremental Encoder Switch 11.7x13.75mm Metal Shaft with bushing

&lt;br&gt;
&lt;br&gt;
Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	Aluminium Alloy
&lt;br&gt;Frame Material	PBT
&lt;br&gt;Frame Flammability Rating	UL94 HB
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Silver
&lt;br&gt;Frame Color	Black
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;Packaging Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;IR	10 mA
&lt;BR&gt;VR	5 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	300 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Electrical Life Encoder	15000 Cycles
&lt;BR&gt;Electrical Life Switch	20000 Cycles
&lt;BR&gt;Detent	16 Positions; 20 Positions; 30 Positions
&lt;BR&gt;Torque Encoder	20 mN*m
&lt;BR&gt;Operation Force (Value)	600 g
&lt;BR&gt;Travel	0.5 mm
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o127908v209%20Family_WS-ENTV_482020714001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o127908v209%20Family_WS-ENTV_482020714001.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/ENTV_11X13_75X26_6_THT_SHAFT_WITH_BUSHING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/ENTV_11X13_75X26_6_THT_SHAFT_WITH_BUSHING&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-05-29&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ENTV_482009514001"/>
</gates>
<devices>
<device name="" package="WS-ENTV_4820XX514001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="COM" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/482009514001?ae"/>
<attribute name="DETENT" value="16 Positions"/>
<attribute name="ELECTRICAL-LIFE-ENCODER" value="15000 Cycles"/>
<attribute name="ELECTRICAL-LIFE-SWITCH" value="20000 Cycles"/>
<attribute name="PART-NUMBER" value="482009514001"/>
<attribute name="RESOLUTION" value="8 Pulse/360 degree"/>
<attribute name="VALUE" value="482009514001"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="482020514001" prefix="S">
<description>&lt;b&gt;WS-ENTV Mechanical Incremental Encoder Switch 11.7x13.75mm Metal Shaft with bushing

&lt;br&gt;
&lt;br&gt;
Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	Aluminium Alloy
&lt;br&gt;Frame Material	PBT
&lt;br&gt;Frame Flammability Rating	UL94 HB
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Silver
&lt;br&gt;Frame Color	Black
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;Packaging Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;IR	10 mA
&lt;BR&gt;VR	5 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	300 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Electrical Life Encoder	15000 Cycles
&lt;BR&gt;Electrical Life Switch	20000 Cycles
&lt;BR&gt;Detent	16 Positions; 20 Positions; 30 Positions
&lt;BR&gt;Torque Encoder	20 mN*m
&lt;BR&gt;Operation Force (Value)	600 g
&lt;BR&gt;Travel	0.5 mm
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o127908v209%20Family_WS-ENTV_482020714001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o127908v209%20Family_WS-ENTV_482020714001.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/ENTV_11X13_75X26_6_THT_SHAFT_WITH_BUSHING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/ENTV_11X13_75X26_6_THT_SHAFT_WITH_BUSHING&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-05-29&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ENTV_482020514001"/>
</gates>
<devices>
<device name="" package="WS-ENTV_4820XX514001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="COM" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/482020514001?ae"/>
<attribute name="DETENT" value="20 Positions"/>
<attribute name="ELECTRICAL-LIFE-ENCODER" value="15000 Cycles"/>
<attribute name="ELECTRICAL-LIFE-SWITCH" value="20000 Cycles"/>
<attribute name="PART-NUMBER" value="482020514001"/>
<attribute name="RESOLUTION" value="20 Pulse/360 degree"/>
<attribute name="VALUE" value="482020514001"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="482012714003" prefix="S">
<description>&lt;b&gt;WS-ENTV Mechanical Incremental Encoder Switch 12.4x13.20mm Plastic Shaft with Threaded bushing

&lt;br&gt;
&lt;br&gt;
Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	PC
&lt;br&gt;Actuator Flammability Rating	UL94 HB
&lt;br&gt;Actuator Color	Black
&lt;br&gt;Frame Material	PBT
&lt;br&gt;Frame Flammability Rating	UL94 HB
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Silver
&lt;br&gt;Frame Color	Black
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;Packaging Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;IR	10 mA
&lt;BR&gt;VR	5 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	300 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Electrical Life Encoder	30000 Cycles
&lt;BR&gt;Electrical Life Switch	20000 Cycles
&lt;BR&gt;Detent	12 Positions
&lt;BR&gt;Torque Encoder	20 mN*m
&lt;BR&gt;Operation Force (Value)	300 g
&lt;BR&gt;Travel	0.5 mm
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o343309v209%20Family_WS-ENTV_4820xx714003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o343309v209%20Family_WS-ENTV_4820xx714003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ENTV_MECHANICAL_INCREMENTAL_ENCODER_SWITCH_12_4_13_2_METAL_THREADED_BUSHING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WS_ENTV_MECHANICAL_INCREMENTAL_ENCODER_SWITCH_12_4_13_2_METAL_THREADED_BUSHING&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-05-29&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ENTV_482012714003"/>
</gates>
<devices>
<device name="" package="WS-ENTV_4820XX714003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="COM" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/482012714003?ae"/>
<attribute name="DETENT" value="12 Positions"/>
<attribute name="ELECTRICAL-LIFE-ENCODER" value="30000 Cycles"/>
<attribute name="ELECTRICAL-LIFE-SWITCH" value="20000 Cycles"/>
<attribute name="PART-NUMBER" value="482012714003"/>
<attribute name="RESOLUTION" value="12 Pulse/360 degree"/>
<attribute name="VALUE" value="482012714003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="482016514001" prefix="S">
<description>&lt;b&gt;WS-ENTV Mechanical Incremental Encoder Switch 11.7x13.75mm Metal Shaft with bushing

&lt;br&gt;
&lt;br&gt;
Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	Aluminium Alloy
&lt;br&gt;Frame Material	PBT
&lt;br&gt;Frame Flammability Rating	UL94 HB
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Silver
&lt;br&gt;Frame Color	Black
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;Packaging Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;IR	10 mA
&lt;BR&gt;VR	5 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	300 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Electrical Life Encoder	15000 Cycles
&lt;BR&gt;Electrical Life Switch	20000 Cycles
&lt;BR&gt;Detent	16 Positions; 20 Positions; 30 Positions
&lt;BR&gt;Torque Encoder	20 mN*m
&lt;BR&gt;Operation Force (Value)	600 g
&lt;BR&gt;Travel	0.5 mm
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o127908v209%20Family_WS-ENTV_482020714001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o127908v209%20Family_WS-ENTV_482020714001.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/ENTV_11X13_75X26_6_THT_SHAFT_WITH_BUSHING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/ENTV_11X13_75X26_6_THT_SHAFT_WITH_BUSHING&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-05-29&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ENTV_482016514001"/>
</gates>
<devices>
<device name="" package="WS-ENTV_4820XX514001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="COM" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/482016514001?ae"/>
<attribute name="DETENT" value="30 Positions"/>
<attribute name="ELECTRICAL-LIFE-ENCODER" value="15000 Cycles"/>
<attribute name="ELECTRICAL-LIFE-SWITCH" value="20000 Cycles"/>
<attribute name="PART-NUMBER" value="482016514001"/>
<attribute name="RESOLUTION" value="15 Pulse/360 degree"/>
<attribute name="VALUE" value="482016514001"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="482016564002" prefix="S">
<description>&lt;b&gt;WS-ENTV Mechanical Incremental Encoder Switch 12.4x13.20mm Plastic Shaft without bushing

&lt;br&gt;
&lt;br&gt;
Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	Aluminium Alloy
&lt;br&gt;Frame Material	LCP
&lt;br&gt;Frame Flammability Rating	UL94 V-0
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Silver
&lt;br&gt;Frame Color	Black
&lt;br&gt;Terminal Material	Copper Alloy
&lt;br&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;Packaging Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;IR	10 mA
&lt;BR&gt;VR	5 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	300 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Electrical Life Encoder	15000 Cycles
&lt;BR&gt;Electrical Life Switch	20000 Cycles
&lt;BR&gt;Detent	30 Positions
&lt;BR&gt;Torque Encoder	20 mN*m
&lt;BR&gt;Operation Force (Value)	350 g
&lt;BR&gt;Travel	0.5 mm
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o343305v209%20Family_WS-ENTV_482016564002.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o343305v209%20Family_WS-ENTV_482016564002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WS_ENTV_MECHANICAL_INCREMENTAL_ENCODER_SWITCH_11_7_12_METAL_PLAIN_BUSHING/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WS_ENTV_MECHANICAL_INCREMENTAL_ENCODER_SWITCH_11_7_12_METAL_PLAIN_BUSHING&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-05-29&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-ENTV_482016564002"/>
</gates>
<devices>
<device name="" package="WS-ENTV_482016564002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="COM" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/482016564002?ae"/>
<attribute name="DETENT" value="30 Positions"/>
<attribute name="ELECTRICAL-LIFE-ENCODER" value="15000 Cycles"/>
<attribute name="ELECTRICAL-LIFE-SWITCH" value="20000 Cycles"/>
<attribute name="PART-NUMBER" value="482016564002"/>
<attribute name="RESOLUTION" value="15 Pulse/360 degree"/>
<attribute name="VALUE" value="482016564002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
