<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - IIIuminated Switches - WS-TASL&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-02-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik
7</description>
<packages>
<package name="WS-TASL_444XX21025816">
<description>&lt;B&gt;WS-TASL&lt;/B&gt;&lt;BR&gt; SMT Illuminated Tact Switch 6.8 x 4.5 mm</description>
</package>
</packages>
<symbols>
<symbol name="WS-TASL1">
<description>WS-TASL1</description>
<pin name="LED1+" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="LED1-" direction="pas"/>
<pin name="LED2-" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="LED2+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="444RD21025816" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TASL SMT Illuminated Tact Switch 6.8 x 4.5 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Base Material:LCP
Base Flammability Rating:UL94 V-0
Actuator Material:LCP
Actuator Flammability Rating:UL94 V-0
Contact Material:Stainless Steel
Contact Plating:Silver
Terminal Plating:Silver
Contact Resistance:100 mΩ
RISO:100 MΩ
Withstanding Voltage:250 V (AC)
Qty.:3000
Emitting Color:Blue &amp; Blue; Bright Green &amp; Bright Green; Bright Green &amp; Red; Red &amp; Red; Yellow &amp; Yellow
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material:LCP
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1:50 mA
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;Operation Force:160 g
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Reel in ESD Bag
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-25
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASL1"/>
</gates>
<devices>
<device name="" package="WS-TASL_444XX21025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="LED1+" pad="3"/>
<connect gate="G$1" pin="LED1-" pad="4"/>
<connect gate="G$1" pin="LED2+" pad="5"/>
<connect gate="G$1" pin="LED2-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/444RD21025816.pdf"/>
<attribute name="EMITTING-COLOR" value="Bright Green &amp; Red"/>
<attribute name="H" value="2.5mm"/>
<attribute name="PART-NUMBER" value="444RD21025816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="444YD21025816" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TASL SMT Illuminated Tact Switch 6.8 x 4.5 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Base Material:LCP
Base Flammability Rating:UL94 V-0
Actuator Material:LCP
Actuator Flammability Rating:UL94 V-0
Contact Material:Stainless Steel
Contact Plating:Silver
Terminal Plating:Silver
Contact Resistance:100 mΩ
RISO:100 MΩ
Withstanding Voltage:250 V (AC)
Qty.:3000
Emitting Color:Blue &amp; Blue; Bright Green &amp; Bright Green; Bright Green &amp; Red; Red &amp; Red; Yellow &amp; Yellow
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material:LCP
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1:50 mA
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;Operation Force:160 g
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Reel in ESD Bag
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-25
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASL1"/>
</gates>
<devices>
<device name="" package="WS-TASL_444XX21025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="LED1+" pad="3"/>
<connect gate="G$1" pin="LED1-" pad="4"/>
<connect gate="G$1" pin="LED2+" pad="5"/>
<connect gate="G$1" pin="LED2-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/444YD21025816.pdf"/>
<attribute name="EMITTING-COLOR" value="Blue &amp; Blue"/>
<attribute name="H" value="2.5mm"/>
<attribute name="PART-NUMBER" value="444YD21025816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="444VR21025816" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TASL SMT Illuminated Tact Switch 6.8 x 4.5 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Base Material:LCP
Base Flammability Rating:UL94 V-0
Actuator Material:LCP
Actuator Flammability Rating:UL94 V-0
Contact Material:Stainless Steel
Contact Plating:Silver
Terminal Plating:Silver
Contact Resistance:100 mΩ
RISO:100 MΩ
Withstanding Voltage:250 V (AC)
Qty.:3000
Emitting Color:Blue &amp; Blue; Bright Green &amp; Bright Green; Bright Green &amp; Red; Red &amp; Red; Yellow &amp; Yellow
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material:LCP
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1:50 mA
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;Operation Force:160 g
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Reel in ESD Bag
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-25
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASL1"/>
</gates>
<devices>
<device name="" package="WS-TASL_444XX21025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="LED1+" pad="3"/>
<connect gate="G$1" pin="LED1-" pad="4"/>
<connect gate="G$1" pin="LED2+" pad="5"/>
<connect gate="G$1" pin="LED2-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/444VR21025816.pdf"/>
<attribute name="EMITTING-COLOR" value="Bright Green &amp; Bright Green"/>
<attribute name="H" value="2.5mm"/>
<attribute name="PART-NUMBER" value="444VR21025816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="444VD21025816" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TASL SMT Illuminated Tact Switch 6.8 x 4.5 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Base Material:LCP
Base Flammability Rating:UL94 V-0
Actuator Material:LCP
Actuator Flammability Rating:UL94 V-0
Contact Material:Stainless Steel
Contact Plating:Silver
Terminal Plating:Silver
Contact Resistance:100 mΩ
RISO:100 MΩ
Withstanding Voltage:250 V (AC)
Qty.:3000
Emitting Color:Blue &amp; Blue; Bright Green &amp; Bright Green; Bright Green &amp; Red; Red &amp; Red; Yellow &amp; Yellow
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material:LCP
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1:50 mA
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;Operation Force:160 g
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Reel in ESD Bag
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-25
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASL1"/>
</gates>
<devices>
<device name="" package="WS-TASL_444XX21025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="LED1+" pad="3"/>
<connect gate="G$1" pin="LED1-" pad="4"/>
<connect gate="G$1" pin="LED2+" pad="5"/>
<connect gate="G$1" pin="LED2-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/444VD21025816.pdf"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Red"/>
<attribute name="H" value="2.5mm"/>
<attribute name="PART-NUMBER" value="444VD21025816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="444BD21025816" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TASL SMT Illuminated Tact Switch 6.8 x 4.5 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Base Material:LCP
Base Flammability Rating:UL94 V-0
Actuator Material:LCP
Actuator Flammability Rating:UL94 V-0
Contact Material:Stainless Steel
Contact Plating:Silver
Terminal Plating:Silver
Contact Resistance:100 mΩ
RISO:100 MΩ
Withstanding Voltage:250 V (AC)
Qty.:3000
Emitting Color:Blue &amp; Blue; Bright Green &amp; Bright Green; Bright Green &amp; Red; Red &amp; Red; Yellow &amp; Yellow
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material:LCP
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;IR 1:50 mA
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;Operation Force:160 g
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;Packaging :Reel in ESD Bag
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61149v209%20Family_WS_TLS_Illuminated_444xx21025816_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASL_6_8X4_5_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-25
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASL1"/>
</gates>
<devices>
<device name="" package="WS-TASL_444XX21025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="LED1+" pad="3"/>
<connect gate="G$1" pin="LED1-" pad="4"/>
<connect gate="G$1" pin="LED2+" pad="5"/>
<connect gate="G$1" pin="LED2-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/444BD21025816.pdf"/>
<attribute name="EMITTING-COLOR" value="Yellow &amp; Yellow"/>
<attribute name="H" value="2.5mm"/>
<attribute name="PART-NUMBER" value="444BD21025816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
