<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Switches - Tact Switches - SMT &amp; J-Bend Tact Switch - WS-TASV&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-03-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="430172043816">
<description>&lt;B&gt;WS-TASV SMT Tact Switch 12x12 mm</description>
</package>
<package name="430453031836">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm washable J-Bend SMD Tact Switch,4 pins</description>
</package>
<package name="430152050836">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="434123050836">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt;J-Bend SMT Tact Switch 6.0x3.5 mm, 2 pins</description>
</package>
<package name="434111025826">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Tact Switch 6.0x3.8 mm,2 pins</description>
</package>
<package name="430783034816">
<description>&lt;B&gt;WS-TASV WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm 

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;6x6x3.4mm, SMT, 4pins</description>
</package>
<package name="431153015826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;5x5 mm J-Bend SMD Tact Switch with ground terminal, 4 pins</description>
</package>
<package name="430152070836">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430481025816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Washable Tact Switch 6x6 mm ,4 pins</description>
</package>
<package name="431181008816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt; SMT Tact Switch 5x5 mm with ground terminal , 4 pins</description>
</package>
<package name="430471035826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Washable Tact Switch 6x6 mm ,4 pins</description>
</package>
<package name="4301330508X6">
</package>
<package name="430152070826">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="434121043816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x3.5 mm SMD Tact Switch, 2 pins</description>
</package>
<package name="430162043826">
<description>&lt;B&gt;WS-TASV SMT Tact Switch 12x12 mm</description>
</package>
<package name="435151014845">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; SMT Tact Switch 3.0 x 2.6 mm with ground terminal</description>
</package>
<package name="430151005826">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; SMT Tact Switch 4.5x4.5 mm</description>
</package>
<package name="431471031826">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Tact Switch 6x6 mm with ground terminal,4 pins</description>
</package>
<package name="430182070816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="431183015816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;5x5 mm J-Bend SMD Tact Switch with ground terminal, 4 pins</description>
</package>
<package name="434781025816">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT IP67 Tact Switch 6.2 x 4.1 mm,2 pins</description>
</package>
<package name="434123043816">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt;J-Bend SMT Tact Switch 6.0x3.5 mm, 2 pins</description>
</package>
<package name="430473035826">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm washable J-Bend SMD Tact Switch,4 pins</description>
</package>
<package name="430162073826">
<description>&lt;B&gt;WS-TASV SMT Tact Switch 12x12 mm</description>
</package>
<package name="434133025826">
<description>&lt;b&gt; WS-TASV&lt;br&gt;&lt;/b&gt; J-Bend SMT Tact Switch 4.7x3.5 mm</description>
</package>
<package name="434123050816">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt;J-Bend SMT Tact Switch 6.0x3.5 mm, 2 pins</description>
</package>
<package name="434113043826">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt;J-Bend SMT Tact Switch 6.0x3.5 mm, 2 pins</description>
</package>
<package name="434123043836">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt;J-Bend SMT Tact Switch 6.0x3.5 mm, 2 pins</description>
</package>
<package name="430453025836">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm washable J-Bend SMD Tact Switch,4 pins</description>
</package>
<package name="430481031816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Washable Tact Switch 6x6 mm ,4 pins</description>
</package>
<package name="430182043816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="435451019820">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 4.1 x 2.8 mm</description>
</package>
<package name="430483035816">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm washable J-Bend SMD Tact Switch,4 pins</description>
</package>
<package name="434123025826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt; J-Bend SMT Tact Switch 4.2x3.2 mm</description>
</package>
<package name="434123025816">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt;J-Bend SMT Tact Switch 6.0x3.8 mm,2 pins</description>
</package>
<package name="435441019830">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 4.1 x 2.8 mm</description>
</package>
<package name="430152043836">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="431153008826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;5x5 mm J-Bend SMD Tact Switch with ground terminal, 4 pins</description>
</package>
<package name="431183008816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;5x5 mm J-Bend SMD Tact Switch with ground terminal, 4 pins</description>
</package>
<package name="434133025816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt; J-Bend SMT Tact Switch 4.2x3.2 mm</description>
</package>
<package name="430471031826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Washable Tact Switch 6x6 mm ,4 pins</description>
</package>
<package name="434111043826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x3.5 mm SMD Tact Switch, 2 pins</description>
</package>
<package name="434121043836">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x3.5 mm SMD Tact Switch, 2 pins</description>
</package>
<package name="431151015826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt; SMT Tact Switch 5x5 mm with ground terminal , 4 pins</description>
</package>
<package name="430152130826">
</package>
<package name="434121050836">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x3.5 mm SMD Tact Switch, 2 pins</description>
</package>
<package name="431481031816">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Tact Switch 6x6 mm with ground terminal,4 pins</description>
</package>
<package name="430172073816">
<description>&lt;B&gt;WS-TASV SMT Tact Switch 12x12 mm</description>
</package>
<package name="434771025826">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT IP67 Tact Switch 6.2 x 4.1 mm,2 pins</description>
</package>
<package name="434121050816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x3.5 mm SMD Tact Switch, 2 pins</description>
</package>
<package name="430152080826">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430182095816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430181038816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;4.5x4.5 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430182130816">
</package>
<package name="430483031816">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm washable J-Bend SMD Tact Switch,4 pins</description>
</package>
<package name="430181005816">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; SMT Tact Switch 4.5x4.5 mm</description>
</package>
<package name="430471025826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Washable Tact Switch 6x6 mm ,4 pins</description>
</package>
<package name="434111050826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x3.5 mm SMD Tact Switch, 2 pins</description>
</package>
<package name="434113050826">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt;J-Bend SMT Tact Switch 6.0x3.5 mm, 2 pins</description>
</package>
<package name="430152095826">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="434130025817">
</package>
<package name="431471031836">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Tact Switch 6x6 mm with ground terminal,4 pins</description>
</package>
<package name="430753051832">
<description>&lt;B&gt;WS-TASV WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm 

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;6x6x5.1mm, SMT, 4pins</description>
</package>
<package name="434121025816">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Tact Switch 6.0x3.8 mm,2 pins</description>
</package>
<package name="430451035836">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Washable Tact Switch 6x6 mm ,4 pins</description>
</package>
<package name="434130025833">
</package>
<package name="430773034825">
<description>&lt;B&gt;WS-TASV WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm 

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;6x6x3.4mm, SMT, 4pins</description>
</package>
<package name="430152043826">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430783051816">
<description>&lt;B&gt;WS-TASV WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm 

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;6x6x5.1mm, SMT, 4pins</description>
</package>
<package name="435171014816">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; SMT Tact Switch 3.0 x 2.6 mm with ground terminal</description>
</package>
<package name="430483025816">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm washable J-Bend SMD Tact Switch,4 pins</description>
</package>
<package name="430773051825">
<description>&lt;B&gt;WS-TASV WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm 

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;6x6x5.1mm, SMT, 4pins</description>
</package>
<package name="434113025826">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt;J-Bend SMT Tact Switch 6.0x3.8 mm,2 pins</description>
</package>
<package name="430172085816">
<description>&lt;B&gt;WS-TASV SMT Tact Switch 12x12 mm</description>
</package>
<package name="430453035836">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm washable J-Bend SMD Tact Switch,4 pins</description>
</package>
<package name="431181015816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt; SMT Tact Switch 5x5 mm with ground terminal , 4 pins</description>
</package>
<package name="434163025816">
<description>&lt;b&gt; WS-TASV&lt;br&gt;&lt;/b&gt; J-Bend SMT Tact Switch 4.7x3.5 mm</description>
</package>
<package name="434153017835">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;Tact Switch J-Bend SMD version,4Pins</description>
</package>
<package name="430182080816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430473031826">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm washable J-Bend SMD Tact Switch,4 pins</description>
</package>
<package name="430162085826">
<description>&lt;B&gt;WS-TASV SMT Tact Switch 12x12 mm</description>
</package>
<package name="430182050816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430753034832">
<description>&lt;B&gt;WS-TASV WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm 

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;6x6x3.4mm, SMT, 4pins</description>
</package>
<package name="435431019840">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 4.1 x 2.8 mm</description>
</package>
<package name="430152095836">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430152080836">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430451025836">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Washable Tact Switch 6x6 mm ,4 pins</description>
</package>
<package name="430473025826">
<description>&lt;b&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;6x6 mm washable J-Bend SMD Tact Switch,4 pins</description>
</package>
<package name="435151014824">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; SMT Tact Switch 3.0 x 2.6 mm with ground terminal</description>
</package>
<package name="430173003816">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; J-Bend SMT Tact Switch 3.7x3.7 mm,4Pins</description>
</package>
<package name="431151008826">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt; SMT Tact Switch 5x5 mm with ground terminal , 4 pins</description>
</package>
<package name="434130025852">
</package>
<package name="430152050826">
<description>&lt;b&gt;WS-TASV&lt;/b&gt;&lt;br&gt; 6x6 mm SMD Tact Switch,4 pins</description>
</package>
<package name="430451031836">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Washable Tact Switch 6x6 mm ,4 pins</description>
</package>
<package name="430152130836">
</package>
<package name="430481035816">
<description>&lt;B&gt;WS-TASV&lt;/B&gt;&lt;BR&gt;SMT Washable Tact Switch 6x6 mm ,4 pins</description>
</package>
</packages>
<symbols>
<symbol name="WS-TASX_4P1">
<description>WS-TASX,4Pins</description>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="WS-TASX_2P">
<description>WS-TASX,2Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WS-TASX_4P2G">
<description>WS-TASx,4Pins with 2GND</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WS-TASX_4P">
<description>WS-TASx,4Pins</description>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WS-TASX_4P1G1">
<description>WS-TASX,4Pins,1GND</description>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="WS-TASX_4PG1">
<description>WS-TASX,4Pins with 1GND</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WS-TASX_4P1G2">
<description>WS-TASx,4Pins with 2GND</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WS-TASX_4P_1">
<description>WS-TASX,4Pins</description>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="430172043816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	PPA
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 260 g
&lt;BR&gt;Electrical Life	300000 Cycles; 500000 Cycles

&lt;BR&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TASV_12X12_SMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_12X12_SMD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-25
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="&quot;" package="430172043816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430172043816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430172043816"/>
<attribute name="VALUE" value="430172043816"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430453031836" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Washable Tact Switch 6x6 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE//"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-08
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430453031836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430453031836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430453031836"/>
<attribute name="VALUE" value="430453031836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152050836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152050836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152050836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430152050836"/>
<attribute name="VALUE" value="430152050836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434123050836" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 6.0x3.5 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:1Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:1500; 1800
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434123050836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434123050836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="434123050836"/>
<attribute name="VALUE" value="434123050836"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434111025826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6.0x3.8 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black;White
&lt;BR&gt;Frame Material: LCP 
&lt;BR&gt;Frame Flammability Rating :UL94 V-0 
&lt;BR&gt;Frame Color: Black 
&lt;BR&gt;Contact Material :Stainless Steel 
&lt;BR&gt;Contact Plating: Silver 
&lt;BR&gt;Terminal Material: Copper Alloy 
&lt;BR&gt;Terminal Plating: Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial:100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test: 1 Ω 
&lt;BR&gt;RISO:100 MΩ 
&lt;BR&gt;Withstanding Voltage:250 V (AC) 
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:3000

&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37584v209%20Family_WS-TASV_SMD_6.0x3.8_Tact_Switch_4341x10258x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37584v209%20Family_WS-TASV_SMD_6.0x3.8_Tact_Switch_4341x10258x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_8_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_8_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434111025826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434111025826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="30000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="434111025826"/>
<attribute name="VALUE" value="434111025826"/>
<attribute name="WIDTH" value="3.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431153015826" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 5x5 mm with ground terminal &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:15 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o70342v209%20Family_WS-TASV_Normal_SMD_J-Bend_4311x30xx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o70342v209%20Family_WS-TASV_Normal_SMD_J-Bend_4311x30xx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_5X5_J-BEND_SMD_WITH_GROUND_TERMINAL_4311x30xx8x6/"&gt;https://www.we-online.com/catalog/en/TASV_5X5_J-BEND_SMD_WITH_GROUND_TERMINAL_4311x30xx8x6/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P2G"/>
</gates>
<devices>
<device name="" package="431153015826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="GND2"/>
<connect gate="G$1" pin="6" pad="GN1"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431153015826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="431153015826"/>
<attribute name="VALUE" value="431153015826"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430783034816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +85 °C
&lt;BR&gt;Washable	Yes
&lt;BR&gt;Ingress Protection Code	IP67
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Actuator Material	Silicone Rubber
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	HTN
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver

&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 250 g; 320 g
&lt;BR&gt;Electrical Life	200000 Cycles; 500000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TASV_6X6_SMD_J-BEND_HERMETIC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_6X6_SMD_J-BEND_HERMETIC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-12-04&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430783034816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430783034816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="3.4mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430783034816"/>
<attribute name="VALUE" value="430783034816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152070836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152070836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152070836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="7mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430152070836"/>
<attribute name="VALUE" value="430152070836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430481025816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 6x6 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430481025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430481025816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430481025816"/>
<attribute name="VALUE" value="430481025816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431181008816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 5x5 mm with ground terminal &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:15 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o70340v209%20Family_WS-TASV_Normal_SMD_4311x10xx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o70340v209%20Family_WS-TASV_Normal_SMD_4311x10xx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_5X5_SMD_WITH_GROUND_TERMINAL_4311x10xx8x6/"&gt;https://www.we-online.com/catalog/en/TASV_5X5_SMD_WITH_GROUND_TERMINAL_4311x10xx8x6/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P2G"/>
</gates>
<devices>
<device name="" package="431181008816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="GND1"/>
<connect gate="G$1" pin="6" pad="GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431181008816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="431181008816"/>
<attribute name="VALUE" value="431181008816"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430471035826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 6x6 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430471035826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430471035826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430471035826"/>
<attribute name="VALUE" value="430471035826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430133050816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT long travel tact switch 6 x 6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material	PA6T
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	LCP
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +125 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	16 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Operation Force (Value)	160 g
&lt;br&gt;Electrical Life	100000 Cycles

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o719224v209%20family-tasv-4301330508x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o719224v209%20family-tasv-4301330508x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
       
Details see: &lt;a href="www.we-online.com/catalog/WS-TASV_SMT_LONG_TRAVEL_TACT_6X6/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WS-TASV_SMT_LONG_TRAVEL_TACT_6X6&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-15
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="4301330508X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430133050816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="100000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430133050816"/>
<attribute name="VALUE" value="430133050816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434121043816" prefix="S">
<description>&lt;b&gt; WS-TASV SMT Tact Switch 6.0x3.5 mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Black; Salmon; White 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black; White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 1500; 1800 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Stroke  0.25 mm 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434121043816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434121043816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434121043816"/>
<attribute name="VALUE" value="434121043816"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430162043826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	PPA
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 260 g
&lt;BR&gt;Electrical Life	300000 Cycles; 500000 Cycles

&lt;BR&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TASV_12X12_SMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_12X12_SMD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-25
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430162043826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430162043826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="300000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430162043826"/>
<attribute name="VALUE" value="430162043826"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="435151014845" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 3.0 x 2.6 mm with ground terminal
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color White;​ Salmon;​ Black 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 2 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 9500 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o158914v209%20WS-TASV-4351x10148xx_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o158914v209%20WS-TASV-4351x10148xx_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WS_TASV_SMT_TACT_SWITCH_3_x_2_6"&gt;https://katalog.we-online.com/en/em/WS_TASV_SMT_TACT_SWITCH_3_x_2_6&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1G1"/>
</gates>
<devices>
<device name="" package="435151014845">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/435151014845?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="450g"/>
<attribute name="PART-NUMBER" value="435151014845"/>
<attribute name="VALUE" value="435151014845"/>
<attribute name="WIDTH" value="2.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152070826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152070826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152070826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="7mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430152070826"/>
<attribute name="VALUE" value="430152070826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430151005826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 4.5x4.5 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;AFrame Material PA9T 
&lt;BR&gt;Frame Flammability Rating UL94 V-0 
&lt;BR&gt;Frame Color Blue 
&lt;BR&gt;Contact Material Stainless Steel 
&lt;BR&gt;Contact Plating Silver 
&lt;BR&gt;Terminal Material Copper Alloy 
&lt;BR&gt;Terminal Plating Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial 100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test 2 Ω 
&lt;BR&gt;RISO 100 MΩ 
&lt;BR&gt;Withstanding Voltage 250 V (AC) 
&lt;BR&gt;Washable No 
&lt;BR&gt;Qty. 7000 

&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life 200000 Times; 1000000 Times 
&lt;BR&gt;Stroke  0.2 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o158913v209%20WS-TASV-4031x10058x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o158913v209%20WS-TASV-4031x10058x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_4_5_x_4_5/"&gt;https://www.we-online.com/catalog/en/TASV_4_5_x_4_5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430151005826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430151005826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430151005826"/>
<attribute name="VALUE" value="430151005826"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431471031826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm with ground terminal    &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material: LCP 
&lt;BR&gt;Frame Flammability Rating :UL94 V-0 
&lt;BR&gt;Frame Color: Black 
&lt;BR&gt;Contact Material :Stainless Steel 
&lt;BR&gt;Contact Plating: Silver 
&lt;BR&gt;Terminal Material: Copper Alloy 
&lt;BR&gt;Terminal Plating: Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial:100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test: 2 Ω 
&lt;BR&gt;RISO:100 MΩ 
&lt;BR&gt;Withstanding Voltage:250 V (AC) 
&lt;BR&gt;Washable:Yes 
&lt;BR&gt;Qty.:1500 

&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55396v209%20Family_ws-tasw_6x6_SMD_with%20ground%20terminal.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55396v209%20Family_ws-tasw_6x6_SMD_with%20ground%20terminal.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4PG1"/>
</gates>
<devices>
<device name="" package="431471031826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431471031826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="431471031826"/>
<attribute name="VALUE" value="431471031826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430182070816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430182070816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430182070816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="7mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430182070816"/>
<attribute name="VALUE" value="430182070816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431183015816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 5x5 mm with ground terminal &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:15 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o70342v209%20Family_WS-TASV_Normal_SMD_J-Bend_4311x30xx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o70342v209%20Family_WS-TASV_Normal_SMD_J-Bend_4311x30xx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_5X5_J-BEND_SMD_WITH_GROUND_TERMINAL_4311x30xx8x6/"&gt;https://www.we-online.com/catalog/en/TASV_5X5_J-BEND_SMD_WITH_GROUND_TERMINAL_4311x30xx8x6/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P2G"/>
</gates>
<devices>
<device name="" package="431183015816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="GND2"/>
<connect gate="G$1" pin="6" pad="GND1"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431183015816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="431183015816"/>
<attribute name="VALUE" value="431183015816"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434781025816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT IP67 Tact Switch 6.2 x 4.1 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material Stainless Steel 
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material Silicone Rubber 
&lt;BR&gt;Actuator Flammability Rating UL94 HB 
&lt;BR&gt;Actuator Color White 
&lt;BR&gt;Frame Material HTN 
&lt;BR&gt;Frame Flammability Rating UL94 V-0 
&lt;BR&gt;Frame Color Black 
&lt;BR&gt;Contact Material Stainless Steel 
&lt;BR&gt;Contact Plating Silver 
&lt;BR&gt;Terminal Material Copper Alloy 
&lt;BR&gt;Terminal Plating Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial 100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test 2 Ω 
&lt;BR&gt;RISO 100 MΩ 
&lt;BR&gt;Withstanding Voltage 250 V (AC) 
&lt;BR&gt;Washable Yes 


&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life 500000 Cycles 
&lt;BR&gt;Stroke (Value) 0.5 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Washable Yes 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o236238v209%204347x10258x6_group_IP67.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o236238v209%204347x10258x6_group_IP67.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;    
Details see: &lt;a href="https://www.we-online.com/catalog/en/WS-TASV_SMT_IP67_TACT_SWITCH"&gt;https://www.we-online.com/catalog/en/WS-TASV_SMT_IP67_TACT_SWITCH&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2021-01-29
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434781025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434781025816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434781025816"/>
<attribute name="VALUE" value="434781025816"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434123043816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 6.0x3.5 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:1Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:1500; 1800
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434123043816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434123043816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434123043816"/>
<attribute name="VALUE" value="434123043816"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430473035826" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Washable Tact Switch 6x6 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE//"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-08
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430473035826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430473035826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430473035826"/>
<attribute name="VALUE" value="430473035826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430162073826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	PPA
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 260 g
&lt;BR&gt;Electrical Life	300000 Cycles; 500000 Cycles

&lt;BR&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TASV_12X12_SMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_12X12_SMD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-25
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430162073826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430162073826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="300000Cycles"/>
<attribute name="HEIGHT" value="7.3mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430162073826"/>
<attribute name="VALUE" value="430162073826"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434133025826" prefix="S">
<description>&lt;b&gt; WS-TASV J-Bend SMT Tact Switch 4.7x3.5 mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Blue;​ Black 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 15 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 2 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 2500 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o158911v209%20WS-TASV-4341x30258x6_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o158911v209%20WS-TASV-4341x30258x6_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WS_TASV_J_BEND_SMT_4_7_x_3_5/"&gt;https://www.we-online.com/catalog/en/WS_TASV_J_BEND_SMT_4_7_x_3_5/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="434133025826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Blue"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434133025826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="100000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="434133025826"/>
<attribute name="VALUE" value="434133025826"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434123050816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 6.0x3.5 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:1Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:1500; 1800
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434123050816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434123050816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434123050816"/>
<attribute name="VALUE" value="434123050816"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434113043826" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 6.0x3.5 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:1Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:1500; 1800
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434113043826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434113043826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="30000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="434113043826"/>
<attribute name="VALUE" value="434113043826"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430453025836" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Washable Tact Switch 6x6 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE//"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-08
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430453025836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430453025836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430453025836"/>
<attribute name="VALUE" value="430453025836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434123043836" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 6.0x3.5 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:1Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:1500; 1800
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434123043836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434123043836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="434123043836"/>
<attribute name="VALUE" value="434123043836"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430481031816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 6x6 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430481031816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430481031816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430481031816"/>
<attribute name="VALUE" value="430481031816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430182043816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430182043816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430182043816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430182043816"/>
<attribute name="VALUE" value="430182043816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="435451019820" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 4.1 x 2.8 mm 
&lt;br&gt;
&lt;br&gt;
Electrical Properties 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 50 mA 
&lt;br&gt;VR 32 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -55 up to +125 °C 
&lt;br&gt;Washable Yes 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operation Force 200 g; 300 g; 400 g 
&lt;br&gt;Electrical Life 100000 Cycles; 150000 Cycles; 200000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material PA9T 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Frame Material PA9T 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Plating Silver 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o674158v209%20family-ws-tasv-4354x10198x0.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o674158v209%20family-ws-tasv-4354x10198x0.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WS_TASV_SMT_WASHABLE_TACT_SWITCH_4_1_X_2_8"&gt;https://www.we-online.com/catalog/en/WS_TASV_SMT_WASHABLE_TACT_SWITCH_4_1_X_2_8&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-02-08&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1G2"/>
</gates>
<devices>
<device name="" package="435451019820">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/435451019820?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="200g"/>
<attribute name="PART-NUMBER" value="435451019820"/>
<attribute name="VALUE" value="435451019820"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430483035816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Washable Tact Switch 6x6 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE//"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-08
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430483035816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430483035816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430483035816"/>
<attribute name="VALUE" value="430483035816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434123025826" prefix="S">
<description>&lt;b&gt; WS-TASV J-Bend SMT Tact Switch 4.2x3.2 mm 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Black; White 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 16 V (DC) 
&lt;br&gt;Contact Resistance Initial 500 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Qty. 2900 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Stroke  0.2 mm 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o106805v209%20Family_WS-TASV-4341x30258x6_Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o106805v209%20Family_WS-TASV-4341x30258x6_Gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_4_2X3_2_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_4_2X3_2_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="434123025826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434123025826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="434123025826"/>
<attribute name="VALUE" value="434123025826"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="435441019830" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 4.1 x 2.8 mm 
&lt;br&gt;
&lt;br&gt;
Electrical Properties 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 50 mA 
&lt;br&gt;VR 32 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -55 up to +125 °C 
&lt;br&gt;Washable Yes 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operation Force 200 g; 300 g; 400 g 
&lt;br&gt;Electrical Life 100000 Cycles; 150000 Cycles; 200000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material PA9T 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Frame Material PA9T 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Plating Silver 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o674158v209%20family-ws-tasv-4354x10198x0.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o674158v209%20family-ws-tasv-4354x10198x0.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WS_TASV_SMT_WASHABLE_TACT_SWITCH_4_1_X_2_8"&gt;https://www.we-online.com/catalog/en/WS_TASV_SMT_WASHABLE_TACT_SWITCH_4_1_X_2_8&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-02-08&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1G2"/>
</gates>
<devices>
<device name="" package="435441019830">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/435441019830?ae"/>
<attribute name="ELECTRICAL-LIFE" value="150000Cycles"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="300g"/>
<attribute name="PART-NUMBER" value="435441019830"/>
<attribute name="VALUE" value="435441019830"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152043836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152043836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152043836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430152043836"/>
<attribute name="VALUE" value="430152043836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431153008826" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 5x5 mm with ground terminal &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:15 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o70342v209%20Family_WS-TASV_Normal_SMD_J-Bend_4311x30xx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o70342v209%20Family_WS-TASV_Normal_SMD_J-Bend_4311x30xx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_5X5_J-BEND_SMD_WITH_GROUND_TERMINAL_4311x30xx8x6/"&gt;https://www.we-online.com/catalog/en/TASV_5X5_J-BEND_SMD_WITH_GROUND_TERMINAL_4311x30xx8x6/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P2G"/>
</gates>
<devices>
<device name="" package="431153008826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="GND2"/>
<connect gate="G$1" pin="6" pad="GND1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431153008826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="431153008826"/>
<attribute name="VALUE" value="431153008826"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431183008816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 5x5 mm with ground terminal &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:15 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o70342v209%20Family_WS-TASV_Normal_SMD_J-Bend_4311x30xx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o70342v209%20Family_WS-TASV_Normal_SMD_J-Bend_4311x30xx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_5X5_J-BEND_SMD_WITH_GROUND_TERMINAL_4311x30xx8x6/"&gt;https://www.we-online.com/catalog/en/TASV_5X5_J-BEND_SMD_WITH_GROUND_TERMINAL_4311x30xx8x6/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P2G"/>
</gates>
<devices>
<device name="" package="431183008816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="GND2"/>
<connect gate="G$1" pin="6" pad="GND1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431183008816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="431183008816"/>
<attribute name="VALUE" value="431183008816"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434133025816" prefix="S">
<description>&lt;b&gt; WS-TASV J-Bend SMT Tact Switch 4.2x3.2 mm 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Black; White 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 16 V (DC) 
&lt;br&gt;Contact Resistance Initial 500 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Qty. 2900 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Stroke  0.2 mm 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o106805v209%20Family_WS-TASV-4341x30258x6_Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o106805v209%20Family_WS-TASV-4341x30258x6_Gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_4_2X3_2_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_4_2X3_2_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="434133025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434133025816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="100000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434133025816"/>
<attribute name="VALUE" value="434133025816"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430471031826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 6x6 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430471031826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430471031826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430471031826"/>
<attribute name="VALUE" value="430471031826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434111043826" prefix="S">
<description>&lt;b&gt; WS-TASV SMT Tact Switch 6.0x3.5 mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Black; Salmon; White 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black; White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 1500; 1800 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Stroke  0.25 mm 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434111043826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434111043826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="30000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="434111043826"/>
<attribute name="VALUE" value="434111043826"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434121043836" prefix="S">
<description>&lt;b&gt; WS-TASV SMT Tact Switch 6.0x3.5 mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Black; Salmon; White 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black; White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 1500; 1800 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Stroke  0.25 mm 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434121043836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434121043836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="434121043836"/>
<attribute name="VALUE" value="434121043836"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431151015826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 5x5 mm with ground terminal &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:15 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o70340v209%20Family_WS-TASV_Normal_SMD_4311x10xx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o70340v209%20Family_WS-TASV_Normal_SMD_4311x10xx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_5X5_SMD_WITH_GROUND_TERMINAL_4311x10xx8x6/"&gt;https://www.we-online.com/catalog/en/TASV_5X5_SMD_WITH_GROUND_TERMINAL_4311x10xx8x6/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P2G"/>
</gates>
<devices>
<device name="" package="431151015826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="GND1"/>
<connect gate="G$1" pin="6" pad="GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431151015826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="431151015826"/>
<attribute name="VALUE" value="431151015826"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434123025816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 6.0x3.8 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black;White
&lt;BR&gt;Frame Material: LCP 
&lt;BR&gt;Frame Flammability Rating :UL94 V-0 
&lt;BR&gt;Frame Color: Black 
&lt;BR&gt;Contact Material :Stainless Steel 
&lt;BR&gt;Contact Plating: Silver 
&lt;BR&gt;Terminal Material: Copper Alloy 
&lt;BR&gt;Terminal Plating: Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial:100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test: 1 Ω 
&lt;BR&gt;RISO:100 MΩ 
&lt;BR&gt;Withstanding Voltage:250 V (AC) 
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:3000

&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o41273v209%20Family_WS-TASV_J-Bend_SMD_6.0x3.8_J-Bend_Tact_Switch_4341x30258x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o41273v209%20Family_WS-TASV_J-Bend_SMD_6.0x3.8_J-Bend_Tact_Switch_4341x30258x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_8_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_8_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434123025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434123025816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434123025816"/>
<attribute name="VALUE" value="434123025816"/>
<attribute name="WIDTH" value="3.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152130826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	LCP
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Operation Force (Value)	160 g; 260 g; 360 g
&lt;br&gt;Electrical Life	200000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Packaging	Tape and Reel

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
       
Details see: &lt;a href="www.we-online.com/catalog/TASV_6X6_SMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_6X6_SMD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-09-20
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152130826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152130826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430152130826"/>
<attribute name="VALUE" value="430152130826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434121050836" prefix="S">
<description>&lt;b&gt; WS-TASV SMT Tact Switch 6.0x3.5 mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Black; Salmon; White 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black; White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 1500; 1800 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Stroke  0.25 mm 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434121050836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434121050836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="434121050836"/>
<attribute name="VALUE" value="434121050836"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430172073816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	PPA
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 260 g
&lt;BR&gt;Electrical Life	300000 Cycles; 500000 Cycles

&lt;BR&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TASV_12X12_SMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_12X12_SMD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-25
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430172073816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430172073816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="7.3mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430172073816"/>
<attribute name="VALUE" value="430172073816"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431481031816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm with ground terminal    &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material: LCP 
&lt;BR&gt;Frame Flammability Rating :UL94 V-0 
&lt;BR&gt;Frame Color: Black 
&lt;BR&gt;Contact Material :Stainless Steel 
&lt;BR&gt;Contact Plating: Silver 
&lt;BR&gt;Terminal Material: Copper Alloy 
&lt;BR&gt;Terminal Plating: Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial:100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test: 2 Ω 
&lt;BR&gt;RISO:100 MΩ 
&lt;BR&gt;Withstanding Voltage:250 V (AC) 
&lt;BR&gt;Washable:Yes 
&lt;BR&gt;Qty.:1500 

&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55396v209%20Family_ws-tasw_6x6_SMD_with%20ground%20terminal.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55396v209%20Family_ws-tasw_6x6_SMD_with%20ground%20terminal.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4PG1"/>
</gates>
<devices>
<device name="" package="431481031816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431481031816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="431481031816"/>
<attribute name="VALUE" value="431481031816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434771025826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT IP67 Tact Switch 6.2 x 4.1 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material Stainless Steel 
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material Silicone Rubber 
&lt;BR&gt;Actuator Flammability Rating UL94 HB 
&lt;BR&gt;Actuator Color White 
&lt;BR&gt;Frame Material HTN 
&lt;BR&gt;Frame Flammability Rating UL94 V-0 
&lt;BR&gt;Frame Color Black 
&lt;BR&gt;Contact Material Stainless Steel 
&lt;BR&gt;Contact Plating Silver 
&lt;BR&gt;Terminal Material Copper Alloy 
&lt;BR&gt;Terminal Plating Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial 100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test 2 Ω 
&lt;BR&gt;RISO 100 MΩ 
&lt;BR&gt;Withstanding Voltage 250 V (AC) 
&lt;BR&gt;Washable Yes 


&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life 500000 Cycles 
&lt;BR&gt;Stroke (Value) 0.5 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;Washable Yes 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o236238v209%204347x10258x6_group_IP67.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o236238v209%204347x10258x6_group_IP67.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;                
Details see: &lt;a href="https://www.we-online.com/catalog/en/WS-TASV_SMT_IP67_TACT_SWITCH"&gt;https://www.we-online.com/catalog/en/WS-TASV_SMT_IP67_TACT_SWITCH&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2021-01-21
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434771025826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434771025826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="434771025826"/>
<attribute name="VALUE" value="434771025826"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152080826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152080826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152080826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="8mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430152080826"/>
<attribute name="VALUE" value="430152080826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434121050816" prefix="S">
<description>&lt;b&gt; WS-TASV SMT Tact Switch 6.0x3.5 mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Black; Salmon; White 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black; White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 1500; 1800 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Stroke  0.25 mm 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434121050816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434121050816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434121050816"/>
<attribute name="VALUE" value="434121050816"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430181038816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 4.5x4.5 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; 
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black; Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:1800
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.2 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37336v209%20Family_WS-TASV_SMD_Tact_Switch_430181038816.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37336v209%20Family_WS-TASV_SMD_Tact_Switch_430181038816.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_4_5X4_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_4_5X4_5_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430181038816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430181038816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430181038816"/>
<attribute name="VALUE" value="430181038816"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430182095816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430182095816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430182095816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430182095816"/>
<attribute name="VALUE" value="430182095816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430182130816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	LCP
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Operation Force (Value)	160 g; 260 g; 360 g
&lt;br&gt;Electrical Life	200000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Packaging	Tape and Reel

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
       
Details see: &lt;a href="www.we-online.com/catalog/TASV_6X6_SMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_6X6_SMD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-09-20
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430182130816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430182130816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430182130816"/>
<attribute name="VALUE" value="430182130816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430483031816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Washable Tact Switch 6x6 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE//"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-08
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430483031816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430483031816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430483031816"/>
<attribute name="VALUE" value="430483031816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430181005816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 4.5x4.5 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;AFrame Material PA9T 
&lt;BR&gt;Frame Flammability Rating UL94 V-0 
&lt;BR&gt;Frame Color Blue 
&lt;BR&gt;Contact Material Stainless Steel 
&lt;BR&gt;Contact Plating Silver 
&lt;BR&gt;Terminal Material Copper Alloy 
&lt;BR&gt;Terminal Plating Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial 100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test 2 Ω 
&lt;BR&gt;RISO 100 MΩ 
&lt;BR&gt;Withstanding Voltage 250 V (AC) 
&lt;BR&gt;Washable No 
&lt;BR&gt;Qty. 7000 

&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life 200000 Times; 1000000 Times 
&lt;BR&gt;Stroke  0.2 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o158913v209%20WS-TASV-4031x10058x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o158913v209%20WS-TASV-4031x10058x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_4_5_x_4_5/"&gt;https://www.we-online.com/catalog/en/TASV_4_5_x_4_5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430181005816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430181005816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430181005816"/>
<attribute name="VALUE" value="430181005816"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430471025826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 6x6 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430471025826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430471025826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430471025826"/>
<attribute name="VALUE" value="430471025826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434111050826" prefix="S">
<description>&lt;b&gt; WS-TASV SMT Tact Switch 6.0x3.5 mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Black; Salmon; White 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black; White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 1 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 1500; 1800 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Stroke  0.25 mm 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37582v209%20WS-TASV_4341X1XXX8X6_Family.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434111050826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434111050826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="30000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="434111050826"/>
<attribute name="VALUE" value="434111050826"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434113050826" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 6.0x3.5 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:1Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:1500; 1800
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37583v209%20Family_WS-TASV_J-Bend_6.0x3.5_SMD_Tact_Switch_4341x3xxx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_5_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434113050826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434113050826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="30000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="434113050826"/>
<attribute name="VALUE" value="434113050826"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431471031836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm with ground terminal    &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material: LCP 
&lt;BR&gt;Frame Flammability Rating :UL94 V-0 
&lt;BR&gt;Frame Color: Black 
&lt;BR&gt;Contact Material :Stainless Steel 
&lt;BR&gt;Contact Plating: Silver 
&lt;BR&gt;Terminal Material: Copper Alloy 
&lt;BR&gt;Terminal Plating: Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial:100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test: 2 Ω 
&lt;BR&gt;RISO:100 MΩ 
&lt;BR&gt;Withstanding Voltage:250 V (AC) 
&lt;BR&gt;Washable:Yes 
&lt;BR&gt;Qty.:1500 

&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55396v209%20Family_ws-tasw_6x6_SMD_with%20ground%20terminal.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55396v209%20Family_ws-tasw_6x6_SMD_with%20ground%20terminal.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4PG1"/>
</gates>
<devices>
<device name="" package="431471031836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431471031836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="431471031836"/>
<attribute name="VALUE" value="431471031836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434130025817" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 4.5*3.2mm&lt;br&gt;

&lt;br&gt;General Information
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	No
&lt;br&gt;Ingress Protection Code	None

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	50 mA
&lt;br&gt;VR	16 V (DC)
&lt;br&gt;Contact Resistance Initial	100 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Actuator Material	LCP
&lt;br&gt;Actuator Flammability Rating	UL94 V-0
&lt;br&gt;Frame Material	PPA
&lt;br&gt;Frame Flammability Rating	UL94 V-0
&lt;br&gt;Contact Plating	Silver
&lt;br&gt;Terminal Plating	Silver

&lt;b&gt;&lt;br&gt;&lt;br&gt;
Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operation Force (Value)	170 gf; 330 gf; 520 gf
&lt;br&gt;Electrical Life	100000 Cycles

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o818399v209%20model_WS_SwTASV_4341300258xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o818399v209%20model_WS_SwTASV_4341300258xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WS_TASV_SMT_TACT_SWITCH_4_5_3_2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_TASV_SMT_TACT_SWITCH_4_5_3_2&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-10-29 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P_1"/>
</gates>
<devices>
<device name="" package="434130025817">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Grey"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434130025817?ae"/>
<attribute name="ELECTRICAL-LIFE" value="100000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="170gf"/>
<attribute name="PART-NUMBER" value="434130025817"/>
<attribute name="VALUE" value="434130025817"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430753051832" prefix="S">
<description>&lt;b&gt;WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +85 °C
&lt;BR&gt;Washable	Yes
&lt;BR&gt;Ingress Protection Code	IP67
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Actuator Material	Silicone Rubber
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	HTN
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver

&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 250 g; 320 g
&lt;BR&gt;Electrical Life	200000 Cycles; 500000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TASV_6X6_SMD_J-BEND_HERMETIC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_6X6_SMD_J-BEND_HERMETIC&lt;/a&gt;&lt;p&gt;

Created by Ella  2023-12-04&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430753051832">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430753051832?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="320g"/>
<attribute name="PART-NUMBER" value="430753051832"/>
<attribute name="VALUE" value="430753051832"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152095826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152095826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152095826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430152095826"/>
<attribute name="VALUE" value="430152095826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434121025816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6.0x3.8 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black;White
&lt;BR&gt;Frame Material: LCP 
&lt;BR&gt;Frame Flammability Rating :UL94 V-0 
&lt;BR&gt;Frame Color: Black 
&lt;BR&gt;Contact Material :Stainless Steel 
&lt;BR&gt;Contact Plating: Silver 
&lt;BR&gt;Terminal Material: Copper Alloy 
&lt;BR&gt;Terminal Plating: Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial:100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test: 1 Ω 
&lt;BR&gt;RISO:100 MΩ 
&lt;BR&gt;Withstanding Voltage:250 V (AC) 
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:3000

&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37584v209%20Family_WS-TASV_SMD_6.0x3.8_Tact_Switch_4341x10258x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37584v209%20Family_WS-TASV_SMD_6.0x3.8_Tact_Switch_4341x10258x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_8_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_8_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434121025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434121025816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="50000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434121025816"/>
<attribute name="VALUE" value="434121025816"/>
<attribute name="WIDTH" value="3.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430451035836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 6x6 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430451035836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430451035836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430451035836"/>
<attribute name="VALUE" value="430451035836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434130025833" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 4.5*3.2mm&lt;br&gt;

&lt;br&gt;General Information
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	No
&lt;br&gt;Ingress Protection Code	None

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	50 mA
&lt;br&gt;VR	16 V (DC)
&lt;br&gt;Contact Resistance Initial	100 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Actuator Material	LCP
&lt;br&gt;Actuator Flammability Rating	UL94 V-0
&lt;br&gt;Frame Material	PPA
&lt;br&gt;Frame Flammability Rating	UL94 V-0
&lt;br&gt;Contact Plating	Silver
&lt;br&gt;Terminal Plating	Silver

&lt;b&gt;&lt;br&gt;&lt;br&gt;
Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operation Force (Value)	170 gf; 330 gf; 520 gf
&lt;br&gt;Electrical Life	100000 Cycles

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o818399v209%20model_WS_SwTASV_4341300258xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o818399v209%20model_WS_SwTASV_4341300258xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WS_TASV_SMT_TACT_SWITCH_4_5_3_2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_TASV_SMT_TACT_SWITCH_4_5_3_2&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-10-29 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P_1"/>
</gates>
<devices>
<device name="" package="434130025833">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434130025833?ae"/>
<attribute name="ELECTRICAL-LIFE" value="100000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="330gf"/>
<attribute name="PART-NUMBER" value="434130025833"/>
<attribute name="VALUE" value="434130025833"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430773034825" prefix="S">
<description>&lt;b&gt;WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +85 °C
&lt;BR&gt;Washable	Yes
&lt;BR&gt;Ingress Protection Code	IP67
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Actuator Material	Silicone Rubber
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	HTN
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver

&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 250 g; 320 g
&lt;BR&gt;Electrical Life	200000 Cycles; 500000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TASV_6X6_SMD_J-BEND_HERMETIC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_6X6_SMD_J-BEND_HERMETIC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-12-04&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430773034825">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Grey"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430773034825?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="3.4mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="250g"/>
<attribute name="PART-NUMBER" value="430773034825"/>
<attribute name="VALUE" value="430773034825"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430783051816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +85 °C
&lt;BR&gt;Washable	Yes
&lt;BR&gt;Ingress Protection Code	IP67
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Actuator Material	Silicone Rubber
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	HTN
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver

&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 250 g; 320 g
&lt;BR&gt;Electrical Life	200000 Cycles; 500000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TASV_6X6_SMD_J-BEND_HERMETIC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_6X6_SMD_J-BEND_HERMETIC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-12-04&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430783051816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430783051816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430783051816"/>
<attribute name="VALUE" value="430783051816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152043826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152043826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152043826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="4.3mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430152043826"/>
<attribute name="VALUE" value="430152043826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="435171014816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 3.0 x 2.6 mm with ground terminal
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color White;​ Salmon;​ Black 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 2 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 9500 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o158914v209%20WS-TASV-4351x10148xx_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o158914v209%20WS-TASV-4351x10148xx_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WS_TASV_SMT_TACT_SWITCH_3_x_2_6"&gt;https://katalog.we-online.com/en/em/WS_TASV_SMT_TACT_SWITCH_3_x_2_6&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1G1"/>
</gates>
<devices>
<device name="" package="435171014816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/435171014816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="435171014816"/>
<attribute name="VALUE" value="435171014816"/>
<attribute name="WIDTH" value="2.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430483025816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Washable Tact Switch 6x6 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE//"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-08
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430483025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430483025816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430483025816"/>
<attribute name="VALUE" value="430483025816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430773051825" prefix="S">
<description>&lt;b&gt;WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +85 °C
&lt;BR&gt;Washable	Yes
&lt;BR&gt;Ingress Protection Code	IP67
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Actuator Material	Silicone Rubber
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	HTN
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver

&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 250 g; 320 g
&lt;BR&gt;Electrical Life	200000 Cycles; 500000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TASV_6X6_SMD_J-BEND_HERMETIC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_6X6_SMD_J-BEND_HERMETIC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-12-04&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430773051825">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Grey"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430773051825?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="250g"/>
<attribute name="PART-NUMBER" value="430773051825"/>
<attribute name="VALUE" value="430773051825"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434113025826" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 6.0x3.8 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black;White
&lt;BR&gt;Frame Material: LCP 
&lt;BR&gt;Frame Flammability Rating :UL94 V-0 
&lt;BR&gt;Frame Color: Black 
&lt;BR&gt;Contact Material :Stainless Steel 
&lt;BR&gt;Contact Plating: Silver 
&lt;BR&gt;Terminal Material: Copper Alloy 
&lt;BR&gt;Terminal Plating: Silver 
&lt;BR&gt;VR 12 V (DC) 
&lt;BR&gt;Contact Resistance Initial:100 mΩ 
&lt;BR&gt;Contact Resistance After Life Test: 1 Ω 
&lt;BR&gt;RISO:100 MΩ 
&lt;BR&gt;Withstanding Voltage:250 V (AC) 
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:3000

&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o41273v209%20Family_WS-TASV_J-Bend_SMD_6.0x3.8_J-Bend_Tact_Switch_4341x30258x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o41273v209%20Family_WS-TASV_J-Bend_SMD_6.0x3.8_J-Bend_Tact_Switch_4341x30258x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6_0X3_8_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_6_0X3_8_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_2P"/>
</gates>
<devices>
<device name="" package="434113025826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434113025826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="30000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="434113025826"/>
<attribute name="VALUE" value="434113025826"/>
<attribute name="WIDTH" value="3.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430453035836" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Washable Tact Switch 6x6 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE//"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-08
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430453035836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430453035836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430453035836"/>
<attribute name="VALUE" value="430453035836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434163025816" prefix="S">
<description>&lt;b&gt; WS-TASV J-Bend SMT Tact Switch 4.7x3.5 mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color Blue;​ Black 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color White 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 15 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 2 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 2500 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o158911v209%20WS-TASV-4341x30258x6_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o158911v209%20WS-TASV-4341x30258x6_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WS_TASV_J_BEND_SMT_4_7_x_3_5/"&gt;https://www.we-online.com/catalog/en/WS_TASV_J_BEND_SMT_4_7_x_3_5/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun,Shan 2020-02-20&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="434163025816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434163025816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="300000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="434163025816"/>
<attribute name="VALUE" value="434163025816"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430172085816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	PPA
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 260 g
&lt;BR&gt;Electrical Life	300000 Cycles; 500000 Cycles

&lt;BR&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TASV_12X12_SMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_12X12_SMD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-25
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430172085816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430172085816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="8.5mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430172085816"/>
<attribute name="VALUE" value="430172085816"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434153017835" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 3.5x2.9 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Blue
&lt;BR&gt;Frame Material:PA46
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:1 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.15 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o72753v209%20WS-TASU_434331013822_a_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o72753v209%20WS-TASU_434331013822_a_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_3_5X2_9_SMD_J-BEND/"&gt;https://www.we-online.com/catalog/en/TASV_3_5X2_9_SMD_J-BEND/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="434153017835">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Blue"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434153017835?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="1.7mm"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="350g"/>
<attribute name="PART-NUMBER" value="434153017835"/>
<attribute name="VALUE" value="434153017835"/>
<attribute name="WIDTH" value="2.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431181015816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 5x5 mm with ground terminal &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:15 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o70340v209%20Family_WS-TASV_Normal_SMD_4311x10xx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o70340v209%20Family_WS-TASV_Normal_SMD_4311x10xx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_5X5_SMD_WITH_GROUND_TERMINAL_4311x10xx8x6/"&gt;https://www.we-online.com/catalog/en/TASV_5X5_SMD_WITH_GROUND_TERMINAL_4311x10xx8x6/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P2G"/>
</gates>
<devices>
<device name="" package="431181015816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="GND1"/>
<connect gate="G$1" pin="6" pad="GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431181015816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="431181015816"/>
<attribute name="VALUE" value="431181015816"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430182080816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430182080816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430182080816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="8mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430182080816"/>
<attribute name="VALUE" value="430182080816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430473031826" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Washable Tact Switch 6x6 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE//"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-08
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430473031826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430473031826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430473031826"/>
<attribute name="VALUE" value="430473031826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430162085826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;BR&gt;

&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	PPA
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 260 g
&lt;BR&gt;Electrical Life	300000 Cycles; 500000 Cycles

&lt;BR&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o76676v209%20Family_WS-TASV-Gruppe.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TASV_12X12_SMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_12X12_SMD&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-25
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430162085826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430162085826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="300000Cycles"/>
<attribute name="HEIGHT" value="8.5mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430162085826"/>
<attribute name="VALUE" value="430162085826"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430753034832" prefix="S">
<description>&lt;b&gt;WS-TASV J-Hook SMT IP67 Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +85 °C
&lt;BR&gt;Washable	Yes
&lt;BR&gt;Ingress Protection Code	IP67
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Actuator Material	Silicone Rubber
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	HTN
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver

&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Operation Force (Value)	160 g; 250 g; 320 g
&lt;BR&gt;Electrical Life	200000 Cycles; 500000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o94204v209%20Family-WS-TASV-4307x30xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/TASV_6X6_SMD_J-BEND_HERMETIC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_6X6_SMD_J-BEND_HERMETIC&lt;/a&gt;&lt;p&gt;

Created by Ella  2023-12-04&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430753034832">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430753034832?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="3.4mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="320g"/>
<attribute name="PART-NUMBER" value="430753034832"/>
<attribute name="VALUE" value="430753034832"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430182050816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430182050816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430182050816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430182050816"/>
<attribute name="VALUE" value="430182050816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="435431019840" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 4.1 x 2.8 mm 
&lt;br&gt;
&lt;br&gt;
Electrical Properties 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 50 mA 
&lt;br&gt;VR 32 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -55 up to +125 °C 
&lt;br&gt;Washable Yes 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operation Force 200 g; 300 g; 400 g 
&lt;br&gt;Electrical Life 100000 Cycles; 150000 Cycles; 200000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material PA9T 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Frame Material PA9T 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Plating Silver 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o674158v209%20family-ws-tasv-4354x10198x0.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o674158v209%20family-ws-tasv-4354x10198x0.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WS_TASV_SMT_WASHABLE_TACT_SWITCH_4_1_X_2_8"&gt;https://www.we-online.com/catalog/en/WS_TASV_SMT_WASHABLE_TACT_SWITCH_4_1_X_2_8&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2022-02-08&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1G2"/>
</gates>
<devices>
<device name="" package="435431019840">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/435431019840?ae"/>
<attribute name="ELECTRICAL-LIFE" value="100000Cycles"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="400g"/>
<attribute name="PART-NUMBER" value="435431019840"/>
<attribute name="VALUE" value="435431019840"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152095836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152095836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152095836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430152095836"/>
<attribute name="VALUE" value="430152095836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430451025836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 6x6 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430451025836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430451025836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430451025836"/>
<attribute name="VALUE" value="430451025836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152080836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152080836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152080836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="8mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430152080836"/>
<attribute name="VALUE" value="430152080836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430473025826" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Washable Tact Switch 6x6 mm   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37581v209%20Family_WS-TASV_6x6_J-Bend_SMD_Tact_Switch_4304830xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE//"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_J-BEND_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-08
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430473025826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430473025826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430473025826"/>
<attribute name="VALUE" value="430473025826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="435151014824" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 3.0 x 2.6 mm with ground terminal
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Cover Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Actuator Material LCP 
&lt;br&gt;Actuator Flammability Rating UL94 V-0 
&lt;br&gt;Actuator Color White;​ Salmon;​ Black 
&lt;br&gt;Frame Material LCP 
&lt;br&gt;Frame Flammability Rating UL94 V-0 
&lt;br&gt;Frame Color Black 
&lt;br&gt;Contact Material Stainless Steel 
&lt;br&gt;Contact Plating Silver 
&lt;br&gt;Terminal Material Copper Alloy 
&lt;br&gt;Terminal Plating Silver 
&lt;br&gt;VR 12 V (DC) 
&lt;br&gt;Contact Resistance Initial 100 mΩ 
&lt;br&gt;Contact Resistance After Life Test 2 Ω 
&lt;br&gt;RISO 100 MΩ 
&lt;br&gt;Withstanding Voltage 250 V (AC) 
&lt;br&gt;Washable No 
&lt;br&gt;Qty. 9500 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o158914v209%20WS-TASV-4351x10148xx_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o158914v209%20WS-TASV-4351x10148xx_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WS_TASV_SMT_TACT_SWITCH_3_x_2_6"&gt;https://katalog.we-online.com/en/em/WS_TASV_SMT_TACT_SWITCH_3_x_2_6&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1G1"/>
</gates>
<devices>
<device name="" package="435151014824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/435151014824?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="240g"/>
<attribute name="PART-NUMBER" value="435151014824"/>
<attribute name="VALUE" value="435151014824"/>
<attribute name="WIDTH" value="2.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430173003816" prefix="S">
<description>&lt;b&gt;WS-TASV J-Bend SMT Tact Switch 3.7x3.7 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Washable	No

&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Electrical Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;
&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Frame Material	LCP
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operation Force (Value)	160 g
&lt;br&gt;Electrical Life	500000 Cycles
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel
&lt;br&gt;


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o103231v209%20WS-TASV_4301x30038xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o103231v209%20WS-TASV_4301x30038xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TASV_3_7X3_7_SMD_J-BEND/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_3_7X3_7_SMD_J-BEND&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-05-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430173003816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430173003816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="500000Cycles"/>
<attribute name="HEIGHT" value="0.35mm"/>
<attribute name="LENGTH" value="3.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430173003816"/>
<attribute name="VALUE" value="430173003816"/>
<attribute name="WIDTH" value="3.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431151008826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 5x5 mm with ground terminal &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:15 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 1000000 Times
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o70340v209%20Family_WS-TASV_Normal_SMD_4311x10xx8x6.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o70340v209%20Family_WS-TASV_Normal_SMD_4311x10xx8x6.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_5X5_SMD_WITH_GROUND_TERMINAL_4311x10xx8x6/"&gt;https://www.we-online.com/catalog/en/TASV_5X5_SMD_WITH_GROUND_TERMINAL_4311x10xx8x6/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-11-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P2G"/>
</gates>
<devices>
<device name="" package="431151008826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="GND1"/>
<connect gate="G$1" pin="6" pad="GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/431151008826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="431151008826"/>
<attribute name="VALUE" value="431151008826"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152050826" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:LCP
&lt;BR&gt;Flammability Rating:UL94 V-0
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:4000;5000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:400; 550; 1000
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-18
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152050826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152050826?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430152050826"/>
<attribute name="VALUE" value="430152050826"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="434130025852" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 4.5*3.2mm&lt;br&gt;

&lt;br&gt;General Information
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Operating Temperature	-40 °C up to +85 °C
&lt;br&gt;Washable	No
&lt;br&gt;Ingress Protection Code	None

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	50 mA
&lt;br&gt;VR	16 V (DC)
&lt;br&gt;Contact Resistance Initial	100 mΩ
&lt;br&gt;RISO	100 MΩ
&lt;br&gt;Withstanding Voltage	250 V (AC)

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Actuator Material	LCP
&lt;br&gt;Actuator Flammability Rating	UL94 V-0
&lt;br&gt;Frame Material	PPA
&lt;br&gt;Frame Flammability Rating	UL94 V-0
&lt;br&gt;Contact Plating	Silver
&lt;br&gt;Terminal Plating	Silver

&lt;b&gt;&lt;br&gt;&lt;br&gt;
Mechanical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operation Force (Value)	170 gf; 330 gf; 520 gf
&lt;br&gt;Electrical Life	100000 Cycles

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o818399v209%20model_WS_SwTASV_4341300258xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o818399v209%20model_WS_SwTASV_4341300258xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WS_TASV_SMT_TACT_SWITCH_4_5_3_2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WS_TASV_SMT_TACT_SWITCH_4_5_3_2&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-10-29 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P_1"/>
</gates>
<devices>
<device name="" package="434130025852">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="White"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/434130025852?ae"/>
<attribute name="ELECTRICAL-LIFE" value="100000Cycles"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="520gf"/>
<attribute name="PART-NUMBER" value="434130025852"/>
<attribute name="VALUE" value="434130025852"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430451031836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 6x6 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430451031836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430451031836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430451031836"/>
<attribute name="VALUE" value="430451031836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430152130836" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material	LCP
&lt;BR&gt;Actuator Flammability Rating	UL94 V-0
&lt;BR&gt;Frame Material	LCP
&lt;BR&gt;Frame Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;Ingress Protection Code	None
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	50 mA
&lt;BR&gt;VR	12 V (DC)
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	250 V (AC)
&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Mechanical Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Operation Force (Value)	160 g; 260 g; 360 g
&lt;br&gt;Electrical Life	200000 Cycles; 1000000 Cycles

&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Packaging	Tape and Reel

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o37470v209%20Family_WS-TASV_6x6mm_SMD_Tact_Switch_4301820xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
       
Details see: &lt;a href="www.we-online.com/catalog/TASV_6X6_SMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TASV_6X6_SMD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-09-20
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="430152130836">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Salmon"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430152130836?ae"/>
<attribute name="ELECTRICAL-LIFE" value="200000Cycles"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430152130836"/>
<attribute name="VALUE" value="430152130836"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430481035816" prefix="S">
<description>&lt;b&gt;WS-TASV SMT Washable Tact Switch 6x6 mm  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability :UL94 V-0
&lt;BR&gt;Rating
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:2000
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke :0.25 mm&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Tape and Reel

&lt;/b&gt;&lt;br&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o37542v209%20Family_WS-TASV_SMD_Tact_Switch_6x6mm_4304810xx8xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/"&gt;https://www.we-online.com/catalog/en/TASV_6X6_SMD_WASHABLE/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-02-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P"/>
</gates>
<devices>
<device name="" package="430481035816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="ACTUATOR-COLOR" value="Black"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/430481035816?ae"/>
<attribute name="ELECTRICAL-LIFE" value="1000000Cycles"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430481035816"/>
<attribute name="VALUE" value="430481035816"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
