<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Switches - IIIuminated Switches - WS-TATL&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-12-17&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WS-TATL_440XX67082622">
<description>&lt;B&gt;WS-TATL THT Illuminated Tact Switch 12 x 12 mm
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;LXHXH=12X12X8.2mm, THT</description>
</package>
</packages>
<symbols>
<symbol name="WS-TATL">
<description>WS-TATL</description>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WS-TATL_440VR67082622">
<description>WS-TATL</description>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WS-TATL_440M167082622">
<description>WS-TATL</description>
<pin name="1" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="440BS67082622" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATL THT Illuminated Tact Switch 12 x 12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Actuator Material	PA66
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Actuator Color	White
&lt;BR&gt;Base Material	PA66
&lt;BR&gt;Base Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	PA66
&lt;BR&gt;Frame Flammability Rating	UL94 HB
&lt;BR&gt;Frame Color	Black
&lt;BR&gt;Diffuser Plate Flammability Rating	UL94 HB
&lt;BR&gt;LED Terminal Material	Copper Alloy
&lt;BR&gt;LED Terminal Plating	Tin
&lt;BR&gt;Contact Material	Stainless Steel&lt;BR&gt;Z
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Material	Copper Alloy
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	2 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	500 V (AC)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operation Force (Value)	220 g
&lt;BR&gt;Electrical Life	100000 Cycles
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Optical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Lens Type	Water clear; Waterclear
&lt;BR&gt;Chip Technology	AlGaInP; AlGaInP + Gan + InGaN; InGaN
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	ESD Tray
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TATL_12X12_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TATL_12X12_THT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATL"/>
</gates>
<devices>
<device name="" package="WS-TATL_440XX67082622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/440BS67082622?ae"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="HEIGHT" value="8.2mm"/>
<attribute name="PART-NUMBER" value="440BS67082622"/>
<attribute name="VALUE" value="440BS67082622"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="440GS67082622" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATL THT Illuminated Tact Switch 12 x 12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Actuator Material	PA66
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Actuator Color	White
&lt;BR&gt;Base Material	PA66
&lt;BR&gt;Base Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	PA66
&lt;BR&gt;Frame Flammability Rating	UL94 HB
&lt;BR&gt;Frame Color	Black
&lt;BR&gt;Diffuser Plate Flammability Rating	UL94 HB
&lt;BR&gt;LED Terminal Material	Copper Alloy
&lt;BR&gt;LED Terminal Plating	Tin
&lt;BR&gt;Contact Material	Stainless Steel&lt;BR&gt;Z
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Material	Copper Alloy
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	2 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	500 V (AC)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operation Force (Value)	220 g
&lt;BR&gt;Electrical Life	100000 Cycles
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Optical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Lens Type	Water clear; Waterclear
&lt;BR&gt;Chip Technology	AlGaInP; AlGaInP + Gan + InGaN; InGaN
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	ESD Tray
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TATL_12X12_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TATL_12X12_THT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATL"/>
</gates>
<devices>
<device name="" package="WS-TATL_440XX67082622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/440GS67082622?ae"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="HEIGHT" value="8.2mm"/>
<attribute name="PART-NUMBER" value="440GS67082622"/>
<attribute name="VALUE" value="440GS67082622"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="440YS67082622" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATL THT Illuminated Tact Switch 12 x 12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Actuator Material	PA66
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Actuator Color	White
&lt;BR&gt;Base Material	PA66
&lt;BR&gt;Base Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	PA66
&lt;BR&gt;Frame Flammability Rating	UL94 HB
&lt;BR&gt;Frame Color	Black
&lt;BR&gt;Diffuser Plate Flammability Rating	UL94 HB
&lt;BR&gt;LED Terminal Material	Copper Alloy
&lt;BR&gt;LED Terminal Plating	Tin
&lt;BR&gt;Contact Material	Stainless Steel&lt;BR&gt;Z
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Material	Copper Alloy
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	2 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	500 V (AC)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operation Force (Value)	220 g
&lt;BR&gt;Electrical Life	100000 Cycles
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Optical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Lens Type	Water clear; Waterclear
&lt;BR&gt;Chip Technology	AlGaInP; AlGaInP + Gan + InGaN; InGaN
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	ESD Tray
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TATL_12X12_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TATL_12X12_THT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATL"/>
</gates>
<devices>
<device name="" package="WS-TATL_440XX67082622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/440YS67082622?ae"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="HEIGHT" value="8.2mm"/>
<attribute name="PART-NUMBER" value="440YS67082622"/>
<attribute name="VALUE" value="440YS67082622"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="440RS67082622" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATL THT Illuminated Tact Switch 12 x 12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Actuator Material	PA66
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Actuator Color	White
&lt;BR&gt;Base Material	PA66
&lt;BR&gt;Base Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	PA66
&lt;BR&gt;Frame Flammability Rating	UL94 HB
&lt;BR&gt;Frame Color	Black
&lt;BR&gt;Diffuser Plate Flammability Rating	UL94 HB
&lt;BR&gt;LED Terminal Material	Copper Alloy
&lt;BR&gt;LED Terminal Plating	Tin
&lt;BR&gt;Contact Material	Stainless Steel&lt;BR&gt;Z
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Material	Copper Alloy
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	2 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	500 V (AC)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operation Force (Value)	220 g
&lt;BR&gt;Electrical Life	100000 Cycles
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Optical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Lens Type	Water clear; Waterclear
&lt;BR&gt;Chip Technology	AlGaInP; AlGaInP + Gan + InGaN; InGaN
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	ESD Tray
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TATL_12X12_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TATL_12X12_THT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATL"/>
</gates>
<devices>
<device name="" package="WS-TATL_440XX67082622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/440RS67082622?ae"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="HEIGHT" value="8.2mm"/>
<attribute name="PART-NUMBER" value="440RS67082622"/>
<attribute name="VALUE" value="440RS67082622"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="440VR67082622" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATL THT Illuminated Tact Switch 12 x 12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Actuator Material	PA66
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Actuator Color	White
&lt;BR&gt;Base Material	PA66
&lt;BR&gt;Base Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	PA66
&lt;BR&gt;Frame Flammability Rating	UL94 HB
&lt;BR&gt;Frame Color	Black
&lt;BR&gt;Diffuser Plate Flammability Rating	UL94 HB
&lt;BR&gt;LED Terminal Material	Copper Alloy
&lt;BR&gt;LED Terminal Plating	Tin
&lt;BR&gt;Contact Material	Stainless Steel&lt;BR&gt;Z
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Material	Copper Alloy
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	2 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	500 V (AC)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operation Force (Value)	220 g
&lt;BR&gt;Electrical Life	100000 Cycles
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Optical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Lens Type	Water clear; Waterclear
&lt;BR&gt;Chip Technology	AlGaInP; AlGaInP + Gan + InGaN; InGaN
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	ESD Tray
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TATL_12X12_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TATL_12X12_THT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATL_440VR67082622"/>
</gates>
<devices>
<device name="" package="WS-TATL_440XX67082622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/440VR67082622?ae"/>
<attribute name="EMITTING-COLOR" value="Bright Green &amp; Red"/>
<attribute name="HEIGHT" value="8.2mm"/>
<attribute name="PART-NUMBER" value="440VR67082622"/>
<attribute name="VALUE" value="440VR67082622"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="440M167082622" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATL THT Illuminated Tact Switch 12 x 12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Actuator Material	PA66
&lt;BR&gt;Actuator Flammability Rating	UL94 HB
&lt;BR&gt;Actuator Color	White
&lt;BR&gt;Base Material	PA66
&lt;BR&gt;Base Flammability Rating	UL94 HB
&lt;BR&gt;Frame Material	PA66
&lt;BR&gt;Frame Flammability Rating	UL94 HB
&lt;BR&gt;Frame Color	Black
&lt;BR&gt;Diffuser Plate Flammability Rating	UL94 HB
&lt;BR&gt;LED Terminal Material	Copper Alloy
&lt;BR&gt;LED Terminal Plating	Tin
&lt;BR&gt;Contact Material	Stainless Steel&lt;BR&gt;Z
&lt;BR&gt;Contact Plating	Silver
&lt;BR&gt;Terminal Material	Copper Alloy
&lt;BR&gt;Terminal Plating	Silver
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Contact Resistance Initial	100 mΩ
&lt;BR&gt;Contact Resistance After Life Test	2 Ω
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;Withstanding Voltage	500 V (AC)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Mechanical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operation Force (Value)	220 g
&lt;BR&gt;Electrical Life	100000 Cycles
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Optical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Lens Type	Water clear; Waterclear
&lt;BR&gt;Chip Technology	AlGaInP; AlGaInP + Gan + InGaN; InGaN
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	ESD Tray
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +85 °C
&lt;BR&gt;&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o61151v209%20Family_WS_TLT_Illuminated_440xx67082622_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/TATL_12X12_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/TATL_12X12_THT&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATL_440M167082622"/>
</gates>
<devices>
<device name="" package="WS-TATL_440XX67082622">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/440M167082622?ae"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="HEIGHT" value="8.2mm"/>
<attribute name="PART-NUMBER" value="440M167082622"/>
<attribute name="VALUE" value="440M167082622"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
