<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - Tact Switches - WS-TATU&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-02-21&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="4312560387X6">
<description>&lt;b&gt;WS-TATU&lt;/b&gt;&lt;br&gt; THT Tact Switch 6x6 mm Right Angled Type with ground terminal</description>
</package>
<package name="4312560837X6">
<description>&lt;b&gt;WS-TATU&lt;/b&gt;&lt;br&gt; THT Tact Switch 6x6 mm Right Angled Type with ground terminal</description>
</package>
<package name="4312560587X6">
<description>&lt;b&gt;WS-TATU&lt;/b&gt;&lt;br&gt; THT Tact Switch 6x6 mm Right Angled Type with ground terminal</description>
</package>
<package name="4312560317X6">
<description>&lt;b&gt;WS-TATU&lt;/b&gt;&lt;br&gt; THT Tact Switch 6x6 mm Right Angled Type with ground terminal</description>
</package>
</packages>
<symbols>
<symbol name="WS-TATU">
<description>WS-TATU</description>
<pin name="GND" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="GND1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="431256038726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560387X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256038726.pdf"/>
<attribute name="H" value="3.85mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="431256038726"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256038716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560387X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256038716.pdf"/>
<attribute name="H" value="3.85mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="431256038716"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256038736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560387X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256038736.pdf"/>
<attribute name="H" value="3.85mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="431256038736"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256083736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560837X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4" route="any"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256083736.pdf"/>
<attribute name="H" value="8.35mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="431256083736"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256058726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560587X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256058726.pdf"/>
<attribute name="H" value="5.85mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="431256058726"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256058736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560587X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256058736.pdf"/>
<attribute name="H" value="5.85mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="431256058736"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256083716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560837X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256083716.pdf"/>
<attribute name="H" value="8.35mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="431256083716"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256083726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560837X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256083726.pdf"/>
<attribute name="H" value="8.35mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="431256083726"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256058716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560587X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256058716.pdf"/>
<attribute name="H" value="5.85mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="431256058716"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256031726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560317X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256031726.pdf"/>
<attribute name="H" value="3.15mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="431256031726"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256031736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560317X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4" route="any"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256031736.pdf"/>
<attribute name="H" value="3.15mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="431256031736"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="431256031716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Carbon Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Qty.:500
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61137v209%20Family_WS_TST_THT_4312560xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/"&gt;https://www.we-online.com/catalog/en/TATU_6X6_THT_RIGHT_ANGLED_WITH_GROUND_TERMINAL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TATU"/>
</gates>
<devices>
<device name="" package="4312560317X6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/431256031716.pdf"/>
<attribute name="H" value="3.15mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="431256031716"/>
<attribute name="QTY" value=" 500 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
