<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Single Coil Power Inductors - WE-CHSA&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-05-13&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CHSA_8090">
<description>&lt;B&gt;WE-CHSA SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 8090
&lt;BR&gt;L X W X H = 8.1mm X 8.1mm X 9mm</description>
</package>
<package name="WE-CHSA_1212">
<description>&lt;B&gt;WE-CHSA SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 1212
&lt;BR&gt;L X W X H = 12.2mm X 12.2mm X 11.75mm</description>
</package>
<package name="WE-CHSA_1011">
<description>&lt;B&gt;WE-CHSA SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 1011
&lt;BR&gt;L X W X H = 10.6mm X 10.6mm X 11mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CHSA_1212" prefix="L">
<description>&lt;b&gt;WE-CHSA SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;br&gt;Operating temperature: -55°C to +150°C
&lt;br&gt;Current capability up to 28A
&lt;br&gt;Ideal coplanarity due to embedded solder pads
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;br&gt;Car infotainment
&lt;br&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/xo107952v209,P20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg.pagespeed.ic.AyH6nYZeiv.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/xo107952v209,P20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg.pagespeed.ic.AyH6nYZeiv.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-CHSA"&gt;https://www.we-online.com/catalog/en/WE-CHSA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2021-05-13&lt;br&gt;
2021 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_1212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843320039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843320039.pdf"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="28A"/>
<attribute name="ISAT" value="57A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843320039 "/>
<attribute name="RDC-MAX" value="1.65mohm"/>
<attribute name="RDC-TYPE" value="1.35mohm"/>
<attribute name="VALUE" value="0.39uH"/>
</technology>
<technology name="_7843320068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843320068.pdf"/>
<attribute name="FRES" value="88MHz"/>
<attribute name="IR" value="25.3A"/>
<attribute name="ISAT" value="41.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843320068 "/>
<attribute name="RDC-MAX" value="2.05mohm"/>
<attribute name="RDC-TYPE" value="1.7mohm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_7843320100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843320100.pdf"/>
<attribute name="FRES" value="81MHz"/>
<attribute name="IR" value="22.5A"/>
<attribute name="ISAT" value="33.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843320100 "/>
<attribute name="RDC-MAX" value="2.4mohm"/>
<attribute name="RDC-TYPE" value="2mohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7843320150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843320150.pdf"/>
<attribute name="FRES" value="74MHz"/>
<attribute name="IR" value="19.7A"/>
<attribute name="ISAT" value="28.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843320150 "/>
<attribute name="RDC-MAX" value="3.3mohm"/>
<attribute name="RDC-TYPE" value="2.7mohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7843320270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843320270.pdf"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="16.2A"/>
<attribute name="ISAT" value="21.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843320270 "/>
<attribute name="RDC-MAX" value="4.7mohm"/>
<attribute name="RDC-TYPE" value="3.9mohm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_7843320330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843320330.pdf"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="13.8A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843320330 "/>
<attribute name="RDC-MAX" value="6.4mohm"/>
<attribute name="RDC-TYPE" value="5.3mohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7843320470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843320470.pdf"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="12.2A"/>
<attribute name="ISAT" value="15.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843320470 "/>
<attribute name="RDC-MAX" value="8.2mohm"/>
<attribute name="RDC-TYPE" value="6.85mohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7843320680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843320680.pdf"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="9.8A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843320680 "/>
<attribute name="RDC-MAX" value="11.9mohm"/>
<attribute name="RDC-TYPE" value="9.9mohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7843320820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843320820.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="8.8A"/>
<attribute name="ISAT" value="12.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843320820 "/>
<attribute name="RDC-MAX" value="15mohm"/>
<attribute name="RDC-TYPE" value="12.45mohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7843321000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843321000.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="7.8A"/>
<attribute name="ISAT" value="10.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843321000 "/>
<attribute name="RDC-MAX" value="20.35mohm"/>
<attribute name="RDC-TYPE" value="16.95mohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7843321200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843321200.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="7.1A"/>
<attribute name="ISAT" value="10.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843321200 "/>
<attribute name="RDC-MAX" value="21.5mohm"/>
<attribute name="RDC-TYPE" value="17.9mohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_7843321800">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843321800.pdf"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="5.5A"/>
<attribute name="ISAT" value="7.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843321800 "/>
<attribute name="RDC-MAX" value="38.4mohm"/>
<attribute name="RDC-TYPE" value="32mohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_7843322000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843322000.pdf"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="5.4A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843322000 "/>
<attribute name="RDC-MAX" value="43.1mohm"/>
<attribute name="RDC-TYPE" value="35.9mohm"/>
<attribute name="VALUE" value="20uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CHSA_8090" prefix="L">
<description>&lt;b&gt;WE-CHSA SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;br&gt;Operating temperature: -55°C to +150°C
&lt;br&gt;Current capability up to 28A
&lt;br&gt;Ideal coplanarity due to embedded solder pads
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;br&gt;Car infotainment
&lt;br&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/xo107952v209,P20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg.pagespeed.ic.AyH6nYZeiv.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/xo107952v209,P20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg.pagespeed.ic.AyH6nYZeiv.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-CHSA"&gt;https://www.we-online.com/catalog/en/WE-CHSA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2021-05-13&lt;br&gt;
2021 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_8090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843340033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843340033.pdf"/>
<attribute name="FRES" value="196MHz"/>
<attribute name="IR" value="21A"/>
<attribute name="ISAT" value="36A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843340033 "/>
<attribute name="RDC-MAX" value="2.1mohm"/>
<attribute name="RDC-TYPE" value="1.75mohm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_7843340047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843340047.pdf"/>
<attribute name="FRES" value="146MHz"/>
<attribute name="IR" value="19A"/>
<attribute name="ISAT" value="29.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843340047 "/>
<attribute name="RDC-MAX" value="2.8mohm"/>
<attribute name="RDC-TYPE" value="2.3mohm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_7843340068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843340068.pdf"/>
<attribute name="FRES" value="132MHz"/>
<attribute name="IR" value="15.6A"/>
<attribute name="ISAT" value="24.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843340068 "/>
<attribute name="RDC-MAX" value="4.1mohm"/>
<attribute name="RDC-TYPE" value="3.45mohm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_7843340100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843340100.pdf"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="12.8A"/>
<attribute name="ISAT" value="21.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843340100 "/>
<attribute name="RDC-MAX" value="5.9mohm"/>
<attribute name="RDC-TYPE" value="4.9mohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7843340220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843340220.pdf"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="8.4A"/>
<attribute name="ISAT" value="14.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843340220 "/>
<attribute name="RDC-MAX" value="12mohm"/>
<attribute name="RDC-TYPE" value="10mohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7843340330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843340330.pdf"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="6.8A"/>
<attribute name="ISAT" value="12.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843340330 "/>
<attribute name="RDC-MAX" value="18.4mohm"/>
<attribute name="RDC-TYPE" value="15.35mohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7843340470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843340470.pdf"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="9.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843340470 "/>
<attribute name="RDC-MAX" value="28.9mohm"/>
<attribute name="RDC-TYPE" value="24.1mohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CHSA_1011" prefix="L">
<description>&lt;b&gt;WE-CHSA SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;br&gt;Operating temperature: -55°C to +150°C
&lt;br&gt;Current capability up to 28A
&lt;br&gt;Ideal coplanarity due to embedded solder pads
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;br&gt;Car infotainment
&lt;br&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/xo107952v209,P20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg.pagespeed.ic.AyH6nYZeiv.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/xo107952v209,P20Family_WE-CHSA_78433xxxx_Gruppe_4C.jpg.pagespeed.ic.AyH6nYZeiv.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-CHSA"&gt;https://www.we-online.com/catalog/en/WE-CHSA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2021-05-13&lt;br&gt;
2021 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_1011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843330033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843330033.pdf"/>
<attribute name="FRES" value="230MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="54.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843330033 "/>
<attribute name="RDC-MAX" value="1.7mohm"/>
<attribute name="RDC-TYPE" value="1.4mohm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_7843330056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843330056.pdf"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="23.5A"/>
<attribute name="ISAT" value="43.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843330056 "/>
<attribute name="RDC-MAX" value="2.05mohm"/>
<attribute name="RDC-TYPE" value="1.7mohm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_7843330100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843330100.pdf"/>
<attribute name="FRES" value="88MHz"/>
<attribute name="IR" value="20.3A"/>
<attribute name="ISAT" value="34.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843330100 "/>
<attribute name="RDC-MAX" value="2.9mohm"/>
<attribute name="RDC-TYPE" value="2.4mohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7843330180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843330180.pdf"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="25.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843330180 "/>
<attribute name="RDC-MAX" value="4.7mohm"/>
<attribute name="RDC-TYPE" value="3.9mohm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_7843330330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843330330.pdf"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="13.8A"/>
<attribute name="ISAT" value="20.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843330330 "/>
<attribute name="RDC-MAX" value="6.5mohm"/>
<attribute name="RDC-TYPE" value="5.4mohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7843330390">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843330390.pdf"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="11.2A"/>
<attribute name="ISAT" value="17.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843330390 "/>
<attribute name="RDC-MAX" value="8.7mohm"/>
<attribute name="RDC-TYPE" value="7.25mohm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_7843330560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843330560.pdf"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="IR" value="9.2A"/>
<attribute name="ISAT" value="14.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843330560 "/>
<attribute name="RDC-MAX" value="13mohm"/>
<attribute name="RDC-TYPE" value="10.85mohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_7843330820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843330820.pdf"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="7.2A"/>
<attribute name="ISAT" value="12.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843330820 "/>
<attribute name="RDC-MAX" value="19.1mohm"/>
<attribute name="RDC-TYPE" value="15.9mohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7843331000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843331000.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="6.7A"/>
<attribute name="ISAT" value="10.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843331000 "/>
<attribute name="RDC-MAX" value="25.8mohm"/>
<attribute name="RDC-TYPE" value="21.5mohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7843331200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843331200.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="5.6A"/>
<attribute name="ISAT" value="9.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843331200 "/>
<attribute name="RDC-MAX" value="33.2mohm"/>
<attribute name="RDC-TYPE" value="27.7mohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_7843331800">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843331800.pdf"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="5.1A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843331800 "/>
<attribute name="RDC-MAX" value="41.1mohm"/>
<attribute name="RDC-TYPE" value="34.25mohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_7843332000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7843332000.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843332000 "/>
<attribute name="RDC-MAX" value="60.9mohm"/>
<attribute name="RDC-TYPE" value="50.8mohm"/>
<attribute name="VALUE" value="20uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
