<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Single Coil Power Inductors - WE-CHSA P&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-02-08&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CHSA_P_8090">
<description>&lt;B&gt;WE-CHSA P Performance SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 8090
&lt;BR&gt;L X W X H = 8.1mm X 8.1mm X 9mm</description>
</package>
<package name="WE-CHSA_P_1212">
<description>&lt;B&gt;WE-CHSA P Performance SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 1212
&lt;BR&gt;L X W X H = 12.2mm X 12.2mm X 11.75mm</description>
</package>
<package name="WE-CHSA_P_1011">
<description>&lt;B&gt;WE-CHSA P Performance SMD High Current Inductor
&lt;BR&gt;&lt;/B&gt;Size : 1011
&lt;BR&gt;L X W X H = 10.6mm X 10.6mm X 11mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CHSA_P_8090" prefix="L">
<description>&lt;b&gt;WE-CHSA P Performance SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;BR&gt;Operating temperature: -55 °C up to +150 °C
&lt;BR&gt;Saturation current up to 48.5 A
&lt;BR&gt;Iron alloy core leads to soft saturation
&lt;BR&gt;AEC-Q200
&lt;BR&gt;Excellent coplanarity due to the plastic base
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;DC/DC converter
&lt;BR&gt;Multimedia applications
&lt;BR&gt;Microprocessor filtering
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o658288v209%20family-we-chsa-p784333xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o658288v209%20family-we-chsa-p784333xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE_CHSA_P"&gt;https://www.we-online.com/catalog/en/WE_CHSA_P&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2022-02-08&lt;br&gt;
2022 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_P_8090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78433490036">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433490036.pdf"/>
<attribute name="FRES" value="218MHz"/>
<attribute name="IR" value="19A"/>
<attribute name="ISAT" value="48.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433490036 "/>
<attribute name="RDC-MAX" value="2.8mOhm"/>
<attribute name="VALUE" value="0.36uH"/>
</technology>
<technology name="_78433490056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433490056.pdf"/>
<attribute name="FRES" value="184MHz"/>
<attribute name="IR" value="15.6A"/>
<attribute name="ISAT" value="40.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433490056 "/>
<attribute name="RDC-MAX" value="4.1mOhm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_78433490075">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433490075.pdf"/>
<attribute name="FRES" value="154MHz"/>
<attribute name="IR" value="12.8A"/>
<attribute name="ISAT" value="34.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433490075 "/>
<attribute name="RDC-MAX" value="5.9mOhm"/>
<attribute name="VALUE" value="0.75uH"/>
</technology>
<technology name="_78433490160">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433490160.pdf"/>
<attribute name="FRES" value="93MHz"/>
<attribute name="IR" value="8.4A"/>
<attribute name="ISAT" value="22.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433490160 "/>
<attribute name="RDC-MAX" value="12mOhm"/>
<attribute name="VALUE" value="1.6uH"/>
</technology>
<technology name="_78433490240">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433490240.pdf"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="6.8A"/>
<attribute name="ISAT" value="18.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433490240 "/>
<attribute name="RDC-MAX" value="18.4mOhm"/>
<attribute name="VALUE" value="2.4uH"/>
</technology>
<technology name="_78433490390">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433490390.pdf"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="14.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433490390 "/>
<attribute name="RDC-MAX" value="28.9mOhm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CHSA_P_1212" prefix="L">
<description>&lt;b&gt;WE-CHSA P Performance SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;BR&gt;Operating temperature: -55 °C up to +150 °C
&lt;BR&gt;Saturation current up to 48.5 A
&lt;BR&gt;Iron alloy core leads to soft saturation
&lt;BR&gt;AEC-Q200
&lt;BR&gt;Excellent coplanarity due to the plastic base
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;DC/DC converter
&lt;BR&gt;Multimedia applications
&lt;BR&gt;Microprocessor filtering
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o658288v209%20family-we-chsa-p784333xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o658288v209%20family-we-chsa-p784333xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE_CHSA_P"&gt;https://www.we-online.com/catalog/en/WE_CHSA_P&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2022-02-08&lt;br&gt;
2022 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_P_1212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78433290200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433290200.pdf"/>
<attribute name="FRES" value="64MHz"/>
<attribute name="IR" value="16.2A"/>
<attribute name="ISAT" value="29A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433290200 "/>
<attribute name="RDC-MAX" value="4.7mOhm"/>
<attribute name="VALUE" value="2uH"/>
</technology>
<technology name="_78433290240">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433290240.pdf"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="13.8A"/>
<attribute name="ISAT" value="24.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433290240 "/>
<attribute name="RDC-MAX" value="6.4mOhm"/>
<attribute name="VALUE" value="2.4uH"/>
</technology>
<technology name="_78433290360">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433290360.pdf"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="12.2A"/>
<attribute name="ISAT" value="20.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433290360 "/>
<attribute name="RDC-MAX" value="8.2mOhm"/>
<attribute name="VALUE" value="3.6uH"/>
</technology>
<technology name="_78433290510">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433290510.pdf"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="9.8A"/>
<attribute name="ISAT" value="17A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433290510 "/>
<attribute name="RDC-MAX" value="11.9mOhm"/>
<attribute name="VALUE" value="5.1uH"/>
</technology>
<technology name="_78433290620">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433290620.pdf"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="8.8A"/>
<attribute name="ISAT" value="16A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433290620 "/>
<attribute name="RDC-MAX" value="15mOhm"/>
<attribute name="VALUE" value="6.2uH"/>
</technology>
<technology name="_78433290750">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433290750.pdf"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="7.8A"/>
<attribute name="ISAT" value="14.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433290750 "/>
<attribute name="RDC-MAX" value="20.35mOhm"/>
<attribute name="VALUE" value="7.5uH"/>
</technology>
<technology name="_78433290820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433290820.pdf"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="7.1A"/>
<attribute name="ISAT" value="13.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433290820 "/>
<attribute name="RDC-MAX" value="21.5mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_78433291500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433291500.pdf"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="5.4A"/>
<attribute name="ISAT" value="9.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433291500 "/>
<attribute name="RDC-MAX" value="43.1mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CHSA_P_1011" prefix="L">
<description>&lt;b&gt;WE-CHSA P Performance SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded rod core inductor
&lt;BR&gt;Operating temperature: -55 °C up to +150 °C
&lt;BR&gt;Saturation current up to 48.5 A
&lt;BR&gt;Iron alloy core leads to soft saturation
&lt;BR&gt;AEC-Q200
&lt;BR&gt;Excellent coplanarity due to the plastic base
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;DC/DC converter
&lt;BR&gt;Multimedia applications
&lt;BR&gt;Microprocessor filtering
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o658288v209%20family-we-chsa-p784333xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o658288v209%20family-we-chsa-p784333xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE_CHSA_P"&gt;https://www.we-online.com/catalog/en/WE_CHSA_P&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2022-02-08&lt;br&gt;
2022 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CHSA_P_1011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78433390150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433390150.pdf"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="37.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433390150 "/>
<attribute name="RDC-MAX" value="4.7mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78433390240">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433390240.pdf"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="13.8A"/>
<attribute name="ISAT" value="28.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433390240 "/>
<attribute name="RDC-MAX" value="6.5mOhm"/>
<attribute name="VALUE" value="2.4uH"/>
</technology>
<technology name="_78433390300">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433390300.pdf"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="11.2A"/>
<attribute name="ISAT" value="26.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433390300 "/>
<attribute name="RDC-MAX" value="8.7mOhm"/>
<attribute name="VALUE" value="3uH"/>
</technology>
<technology name="_78433390430">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433390430.pdf"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="IR" value="9.2A"/>
<attribute name="ISAT" value="20.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433390430 "/>
<attribute name="RDC-MAX" value="13mOhm"/>
<attribute name="VALUE" value="4.3uH"/>
</technology>
<technology name="_78433390620">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433390620.pdf"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="7.2A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433390620 "/>
<attribute name="RDC-MAX" value="19.1mOhm"/>
<attribute name="VALUE" value="6.2uH"/>
</technology>
<technology name="_78433390820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433390820.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="6.7A"/>
<attribute name="ISAT" value="15.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433390820 "/>
<attribute name="RDC-MAX" value="25.8mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_78433391000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433391000.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="5.6A"/>
<attribute name="ISAT" value="14.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433391000 "/>
<attribute name="RDC-MAX" value="33.2mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_78433391500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/78433391500.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="11.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78433391500 "/>
<attribute name="RDC-MAX" value="60.9mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
