<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Single Coil Power Inductors - WE-HCIA&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-11-27&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HCIA_7040">
</package>
<package name="WE-HCIA_7050">
<description>&lt;b&gt;WE-HCIA SMD Flat Wire High Current Inductor 
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;7050, SMT, 2pins
&lt;br&gt;L X W X H = 7mm X 6.9mm X 4.8mm</description>
</package>
<package name="WE-HCIA_7030">
</package>
<package name="WE-HCIA_1050">
<description>&lt;b&gt;WE-HCIA SMD Flat Wire High Current Inductor 
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;1050, SMT, 2pins
&lt;br&gt;L X W X H = 10.5mm X 10.2mm X 4.7mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-HCIA">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HCIA_7040" prefix="L">
<description>&lt;b&gt;WE-HCIA SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -55 °C up to +150 °C
&lt;br&gt;Current capability up to 36 A
&lt;br&gt;AEC-Q200
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489349v209%20Family_WE-HCIA_1050.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489349v209%20Family_WE-HCIA_1050.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCIA&lt;/a&gt;&lt;p&gt;


Created by Ella 2024-11-25&lt;br&gt;
2024 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WE-HCIA"/>
</gates>
<devices>
<device name="" package="WE-HCIA_7040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843110022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843110022?ae"/>
<attribute name="FRES" value="366MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="36.4A"/>
<attribute name="ISAT" value="43.9A"/>
<attribute name="LENGTH" value="6.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843110022"/>
<attribute name="RDC-MAX" value="1.21mOhm"/>
<attribute name="SIZE" value=" 7040 "/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_7843110068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843110068?ae"/>
<attribute name="FRES" value="171MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="20.9A"/>
<attribute name="ISAT" value="24.6A"/>
<attribute name="LENGTH" value="6.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843110068"/>
<attribute name="RDC-MAX" value="3.41mOhm"/>
<attribute name="SIZE" value=" 7040 "/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_7843110100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843110100?ae"/>
<attribute name="FRES" value="134MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="16.8A"/>
<attribute name="ISAT" value="20.2A"/>
<attribute name="LENGTH" value="6.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843110100"/>
<attribute name="RDC-MAX" value="5.06mOhm"/>
<attribute name="SIZE" value=" 7040 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_7843110150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843110150?ae"/>
<attribute name="FRES" value="94MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="13.8A"/>
<attribute name="ISAT" value="15.6A"/>
<attribute name="LENGTH" value="6.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843110150"/>
<attribute name="RDC-MAX" value="7.26mOhm"/>
<attribute name="SIZE" value=" 7040 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_7843110220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843110220?ae"/>
<attribute name="FRES" value="76MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="10.2A"/>
<attribute name="ISAT" value="13.4A"/>
<attribute name="LENGTH" value="6.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843110220"/>
<attribute name="RDC-MAX" value="12.54mOhm"/>
<attribute name="SIZE" value=" 7040 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_7843110330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843110330?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="8.1A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="LENGTH" value="6.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843110330"/>
<attribute name="RDC-MAX" value="18.92mOhm"/>
<attribute name="SIZE" value=" 7040 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_7843110470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843110470?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="7.8A"/>
<attribute name="ISAT" value="9.1A"/>
<attribute name="LENGTH" value="6.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843110470"/>
<attribute name="RDC-MAX" value="21.45mOhm"/>
<attribute name="SIZE" value=" 7040 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCIA_7050" prefix="L">
<description>&lt;b&gt;WE-HCIA SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -55 °C up to +150 °C
&lt;br&gt;Current capability up to 36 A
&lt;br&gt;AEC-Q200
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489349v209%20Family_WE-HCIA_1050.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489349v209%20Family_WE-HCIA_1050.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCIA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2022-11-15&lt;br&gt;
2022 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WE-HCIA"/>
</gates>
<devices>
<device name="" package="WE-HCIA_7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843140047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843140047?ae"/>
<attribute name="FRES" value="292MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IR" value="16.9A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843140047"/>
<attribute name="RDC-MAX" value="1.65mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_784314011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784314011?ae"/>
<attribute name="FRES" value="147MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IR" value="14.7A"/>
<attribute name="ISAT" value="15.2A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784314011"/>
<attribute name="RDC-MAX" value="3.47mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="1.1uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_784314033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784314033?ae"/>
<attribute name="FRES" value="68MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IR" value="9.2A"/>
<attribute name="ISAT" value="8.7A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784314033"/>
<attribute name="RDC-MAX" value="9.62mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_784314049">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784314049?ae"/>
<attribute name="FRES" value="64MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IR" value="7.6A"/>
<attribute name="ISAT" value="7.2A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784314049"/>
<attribute name="RDC-MAX" value="15.85mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="4.9uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_784314065">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784314065?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IR" value="6.3A"/>
<attribute name="ISAT" value="6.4A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784314065"/>
<attribute name="RDC-MAX" value="23.65mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="6.5uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_784314100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784314100?ae"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="HEIGHT" value="4.8mm"/>
<attribute name="IR" value="3.7A"/>
<attribute name="ISAT" value="4.85A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784314100"/>
<attribute name="RDC-MAX" value="33.72mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCIA_7030" prefix="L">
<description>&lt;b&gt;WE-HCIA SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -55 °C up to +150 °C
&lt;br&gt;Current capability up to 36 A
&lt;br&gt;AEC-Q200
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489349v209%20Family_WE-HCIA_1050.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489349v209%20Family_WE-HCIA_1050.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCIA&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-11-25&lt;br&gt;
2024 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WE-HCIA"/>
</gates>
<devices>
<device name="" package="WE-HCIA_7030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843100055">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843100055?ae"/>
<attribute name="FRES" value="189MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="19.2A"/>
<attribute name="ISAT" value="27.7A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843100055"/>
<attribute name="RDC-MAX" value="4.07mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="0.52uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_7843100115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843100115?ae"/>
<attribute name="FRES" value="97MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="11.8A"/>
<attribute name="ISAT" value="18.6A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843100115"/>
<attribute name="RDC-MAX" value="9.46mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="1.15uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_7843100150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843100150?ae"/>
<attribute name="FRES" value="91MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="9.6A"/>
<attribute name="ISAT" value="17.9A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843100150"/>
<attribute name="RDC-MAX" value="13.97mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_7843100200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843100200?ae"/>
<attribute name="FRES" value="88MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="8.7A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843100200"/>
<attribute name="RDC-MAX" value="15.62mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="2uH"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCIA_1050" prefix="L">
<description>&lt;b&gt;WE-HCIA SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded
&lt;br&gt;Flat wire coil for low losses
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -55 °C up to +150 °C
&lt;br&gt;Current capability up to 36 A
&lt;br&gt;AEC-Q200
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;Filter choke for motor electronics
&lt;BR&gt;Car infotainment
&lt;BR&gt;Multimedia applications
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489349v209%20Family_WE-HCIA_1050.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489349v209%20Family_WE-HCIA_1050.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCIA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2022-02-10&lt;br&gt;
2022 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WE-HCIA"/>
</gates>
<devices>
<device name="" package="WE-HCIA_1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843250072">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843250072?ae"/>
<attribute name="FRES" value="103MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="22A"/>
<attribute name="ISAT" value="36.1A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843250072"/>
<attribute name="RDC-MAX" value="1.38mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="0.72uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325012?ae"/>
<attribute name="FRES" value="76MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="20A"/>
<attribute name="ISAT" value="30A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325012"/>
<attribute name="RDC-MAX" value="2.04mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325018?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325018"/>
<attribute name="RDC-MAX" value="3.3mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325024?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="20.7A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325024"/>
<attribute name="RDC-MAX" value="5.4mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="2.4uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325033?ae"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325033"/>
<attribute name="RDC-MAX" value="5.75mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325042">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325042?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="15.7A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325042"/>
<attribute name="RDC-MAX" value="7.8mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="4.2uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325055">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325055?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="14.3A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325055"/>
<attribute name="RDC-MAX" value="9.45mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="5.2uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325065">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325065?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="8.4A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325065"/>
<attribute name="RDC-MAX" value="11.55mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="6.5uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325078">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325078?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325078"/>
<attribute name="RDC-MAX" value="14.4mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="7.8uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325100?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="7.2A"/>
<attribute name="ISAT" value="10.3A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325100"/>
<attribute name="RDC-MAX" value="23.1mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
<technology name="_784325160">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784325160?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="4.7mm"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="7.8A"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784325160"/>
<attribute name="RDC-MAX" value="38mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="16.7uH"/>
<attribute name="WIDTH" value="10.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
