<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - REDCUBE - REDCUBE SMD - WP-SMRT&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020b, 2020-07-17&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WP-SMRT_746600135">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal through-hole
&lt;br&gt;&lt;/b&gt;Inner Diamater = 3.5mm;
&lt;br&gt;Max Height = 3mm</description>
</package>
<package name="WP-SMRT_74660014">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal thread
&lt;br&gt;&lt;/b&gt;Thread M4
&lt;br&gt;Max Height = 3mm</description>
</package>
<package name="WP-SMRT_746600155">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal through-hole
&lt;br&gt;&lt;/b&gt;Inner Diamater = 5.5mm;
&lt;br&gt;Max Height = 3mm</description>
</package>
<package name="WP-SMRT_746600165">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal through-hole
&lt;br&gt;&lt;/b&gt;Inner Diamater = 6.5mm;
&lt;br&gt;Max Height = 5.6mm</description>
</package>
<package name="WP-SMRT_74660015">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal thread
&lt;br&gt;&lt;/b&gt;Thread M5
&lt;br&gt;Max Height = 3mm</description>
</package>
<package name="WP-SMRT_74660013">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal thread
&lt;br&gt;&lt;/b&gt;Thread M3
&lt;br&gt;Max Height = 3mm</description>
</package>
<package name="WP-SMRT_746600145">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal through-hole
&lt;br&gt;&lt;/b&gt;Inner Diamater = 4.5mm;
&lt;br&gt;Max Height = 3mm</description>
</package>
<package name="WP-SMRT_74660016">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal thread
&lt;br&gt;&lt;/b&gt;Thread M6
&lt;br&gt;Max Height = 3mm</description>
</package>
<package name="WP-SMRT_74660016R">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal thread
&lt;br&gt;&lt;/b&gt;Thread M6
&lt;br&gt;Max Height = 3mm</description>
</package>
</packages>
<symbols>
<symbol name="WP-SMRT">
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WP-SMRT_7466001X5" prefix="MP">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal through-hole
&lt;br&gt;
&lt;br&gt;Applications &lt;br&gt;
&lt;br&gt;&lt;/b&gt;Solderable high current Wire-to-Board &amp; Board-to-Board connections with a focus on automated assembl
&lt;br&gt;IMS boards or one layer applications
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Material Brass 
&lt;br&gt;Surface Tin 
&lt;br&gt;Operating Temperature -55 up to +150 °C 
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES&lt;/b&gt;&lt;br&gt;
&lt;br&gt;IR  85 A 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Bulk;​ Tape and Reel &lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135751v209%20Family_WP-SMRT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135751v209%20Family_WP-SMRT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="hhttps://www.we-online.com/catalog/en/WP-SMRT_THROUGH-HOLE/"&gt;https://www.we-online.com/catalog/en/WP-SMRT_THROUGH-HOLE/&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2020-07-17
&lt;br&gt;2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WP-SMRT"/>
</gates>
<devices>
<device name="_746600135" package="WP-SMRT_746600135">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/746600135.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="INNER-DIAMETER" value="3.5mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value=" 746600135 "/>
<attribute name="VALUE" value=" 746600135 "/>
</technology>
</technologies>
</device>
<device name="_746600135R" package="WP-SMRT_746600135">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/746600135R.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="INNER-DIAMETER" value="3.5mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value="746600135R"/>
<attribute name="VALUE" value="746600135R"/>
</technology>
</technologies>
</device>
<device name="_746600145" package="WP-SMRT_746600145">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/746600145.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="INNER-DIAMETER" value="4.5mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value=" 746600145 "/>
<attribute name="VALUE" value=" 746600145 "/>
</technology>
</technologies>
</device>
<device name="_746600145R" package="WP-SMRT_746600145">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/746600145R.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="INNER-DIAMETER" value="4.5mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value="746600145R"/>
<attribute name="VALUE" value="746600145R"/>
</technology>
</technologies>
</device>
<device name="_746600155" package="WP-SMRT_746600155">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/746600155.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="INNER-DIAMETER" value="5.5mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value=" 746600155 "/>
<attribute name="VALUE" value=" 746600155 "/>
</technology>
</technologies>
</device>
<device name="_746600155R" package="WP-SMRT_746600155">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/746600155R.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="INNER-DIAMETER" value="5.5mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value="746600155R"/>
<attribute name="VALUE" value="746600155R"/>
</technology>
</technologies>
</device>
<device name="_746600165" package="WP-SMRT_746600165">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/746600165.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="INNER-DIAMETER" value="6.5mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="12mm"/>
<attribute name="PART-NUMBER" value=" 746600165 "/>
<attribute name="VALUE" value=" 746600165 "/>
</technology>
</technologies>
</device>
<device name="_746600165R" package="WP-SMRT_746600165">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/746600165R.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="INNER-DIAMETER" value="6.5mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="12mm"/>
<attribute name="PART-NUMBER" value="746600165R"/>
<attribute name="VALUE" value="746600165R"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WP-SMRT_7466001X" prefix="MP">
<description>&lt;b&gt;WP-SMRT SMT Reverse with internal thread
&lt;br&gt;
&lt;br&gt;Applications &lt;br&gt;
&lt;br&gt;&lt;/b&gt;Solderable high current Wire-to-Board &amp; Board-to-Board connections with a focus on automated assembly
&lt;br&gt;IMS boards or one layer applications
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Material Brass 
&lt;br&gt;Surface Tin 
&lt;br&gt;Operating Temperature -55 up to +150 °C 
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Bulk;​ Tape and Reel 
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o162358v209%20Family_REDCUBE_74660013.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o162358v209%20Family_REDCUBE_74660013.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WP_SMRT_REDCUBE_SMT_REVERSE_TYPE_WITH_INTERNAL_THREAD/"&gt;https://www.we-online.com/catalog/en/WP_SMRT_REDCUBE_SMT_REVERSE_TYPE_WITH_INTERNAL_THREAD/&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2020-07-17
&lt;br&gt;2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WP-SMRT"/>
</gates>
<devices>
<device name="_74660013" package="WP-SMRT_74660013">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74660013.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value=" 74660013 "/>
<attribute name="THREAD" value="M3"/>
<attribute name="VALUE" value=" 74660013 "/>
</technology>
</technologies>
</device>
<device name="_74660013R" package="WP-SMRT_74660013">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74660013R.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value="74660013R"/>
<attribute name="THREAD" value="M3"/>
<attribute name="VALUE" value="74660013R"/>
</technology>
</technologies>
</device>
<device name="_74660014" package="WP-SMRT_74660014">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74660014.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value=" 74660014 "/>
<attribute name="THREAD" value="M4"/>
<attribute name="VALUE" value=" 74660014 "/>
</technology>
</technologies>
</device>
<device name="_74660014R" package="WP-SMRT_74660014">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74660014R.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value="74660014R"/>
<attribute name="THREAD" value="M4"/>
<attribute name="VALUE" value="74660014R"/>
</technology>
</technologies>
</device>
<device name="_74660015" package="WP-SMRT_74660015">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74660015.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value=" 74660015 "/>
<attribute name="THREAD" value="M5"/>
<attribute name="VALUE" value=" 74660015 "/>
</technology>
</technologies>
</device>
<device name="_74660015R" package="WP-SMRT_74660015">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74660015R.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="10mm"/>
<attribute name="PART-NUMBER" value="74660015R"/>
<attribute name="THREAD" value="M5"/>
<attribute name="VALUE" value="74660015R"/>
</technology>
</technologies>
</device>
<device name="_74660016" package="WP-SMRT_74660016">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74660016.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="12mm"/>
<attribute name="PART-NUMBER" value=" 74660016 "/>
<attribute name="THREAD" value="M6"/>
<attribute name="VALUE" value=" 74660016 "/>
</technology>
</technologies>
</device>
<device name="_74660016R" package="WP-SMRT_74660016R">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74660016R.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="85A"/>
<attribute name="OUTER-DIAMETER" value="12mm"/>
<attribute name="PART-NUMBER" value="74660016R"/>
<attribute name="THREAD" value="M6"/>
<attribute name="VALUE" value="74660016R"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
