<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Resistors - Thick Film Resistors - WRIS-KSKE&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Eagle Version 9, Library Revision 2019a, 2019-09-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WRIS-KSKE_2512_6.3X3.2X0.6(LXWXH)">
<description>&lt;B&gt;WRIS-KSKE Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;General Purpose Current Sensing
&lt;BR&gt;Size : 2512</description>
</package>
<package name="WRIS-KSKE_1206_3.1X1.6X0.6X0.3(LXWXHXPW)">
<description>&lt;B&gt;WRIS-KSKE Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;General Purpose Current Sensing
&lt;BR&gt;Size : 1206</description>
</package>
<package name="WRIS-KSKE_0805_2.0X1.25X0.6(LXWXH)">
<description>&lt;B&gt;WRIS-KSKE Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;General Purpose Current Sensing
&lt;BR&gt;Size : 0805</description>
</package>
<package name="WRIS-KSKE_2010_5.0X2.5X0.6(LXWXH)">
<description>&lt;B&gt;WRIS-KSKE Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;General Purpose Current Sensing
&lt;BR&gt;Size : 2010</description>
</package>
<package name="WRIS-KSKE_0402">
<description>&lt;B&gt;WRIS-KSKE Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;General Purpose Current Sensing
&lt;BR&gt;Size : 0402</description>
</package>
<package name="WRIS-KSKE_0603_1.6X0.8X0.45(LXWXH)">
<description>&lt;B&gt;WRIS-KSKE Thick Film Resistors
&lt;BR&gt;&lt;/B&gt;General Purpose Current Sensing
&lt;BR&gt;Size : 0603</description>
</package>
</packages>
<symbols>
<symbol name="R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WRIS-KSKE_2512" prefix="R">
<description>&lt;b&gt; WRIS-KSKE Thick Film Resistors
&lt;br&gt;General Purpose Current Sensing
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;General purpose current sensing product series Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 50 mΩ ‒ 10 Ω
&lt;br&gt;Resistance tolerance: ±1 %
&lt;br&gt;Rated Power: 0.125 W ‒ 1 W
&lt;br&gt;TCR: ±100; +200; +250; +300 ppm/°C
&lt;br&gt;Operating temperature: -55 ��C up to +155°C
&lt;br&gt;Sizes: 0402 / 0603 / 0805 / 1206 / 2010 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Camera; night vision device
&lt;br&gt;Battery management for mobile phone
&lt;br&gt;Electric motor control
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;L X W X H =Length X Width X Height
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KSKE"&gt;https://katalog.we-online.com/en/pbs/WRIS-KSKE&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_6.3X3.2X0.6" package="WRIS-KSKE_2512_6.3X3.2X0.6(LXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_560050363011">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050363011.pdf"/>
<attribute name="IR" value="1.41A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050363011 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE2512R500F101KAATE0000"/>
<attribute name="VALUE" value="0.5Ohm"/>
</technology>
<technology name="_560050363012">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050363012.pdf"/>
<attribute name="IR" value="0.55A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050363012 "/>
<attribute name="PRATED" value="1W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE25123R30F101KAATE0000"/>
<attribute name="VALUE" value="3.3Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-KSKE_1206" prefix="R">
<description>&lt;b&gt; WRIS-KSKE Thick Film Resistors
&lt;br&gt;General Purpose Current Sensing
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;General purpose current sensing product series Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 50 mΩ ‒ 10 Ω
&lt;br&gt;Resistance tolerance: ±1 %
&lt;br&gt;Rated Power: 0.125 W ‒ 1 W
&lt;br&gt;TCR: ±100; +200; +250; +300 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155°C
&lt;br&gt;Sizes: 0402 / 0603 / 0805 / 1206 / 2010 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Camera; night vision device
&lt;br&gt;Battery management for mobile phone
&lt;br&gt;Electric motor control
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;L X W X H X PW=Length X Width X Height X Pad Width
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KSKE"&gt;https://katalog.we-online.com/en/pbs/WRIS-KSKE&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_3.1X1.6X0.6X0.3" package="WRIS-KSKE_1206_3.1X1.6X0.6X0.3(LXWXHXPW)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_560050332001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050332001.pdf"/>
<attribute name="IR" value="3.16A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050332001 "/>
<attribute name="PRATED" value="0.5W"/>
<attribute name="TCR" value="250ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE1206R050F102LAATP0000"/>
<attribute name="VALUE" value="0.05Ohm"/>
</technology>
<technology name="_560050332011">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050332011.pdf"/>
<attribute name="IR" value="0.38A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050332011 "/>
<attribute name="PRATED" value="0.5W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE12063R30F102KAATP0000"/>
<attribute name="VALUE" value="3.3Ohm"/>
</technology>
<technology name="_560050332013">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050332013.pdf"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050332013 "/>
<attribute name="PRATED" value="0.5W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE1206R500F102KAATP0000"/>
<attribute name="VALUE" value="0.5Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-KSKE_2010" prefix="R">
<description>&lt;b&gt; WRIS-KSKE Thick Film Resistors
&lt;br&gt;General Purpose Current Sensing
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;General purpose current sensing product series Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 50 mΩ ‒ 10 Ω
&lt;br&gt;Resistance tolerance: ±1 %
&lt;br&gt;Rated Power: 0.125 W ‒ 1 W
&lt;br&gt;TCR: ±100; +200; +250; +300 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155°C
&lt;br&gt;Sizes: 0402 / 0603 / 0805 / 1206 / 2010 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Camera; night vision device
&lt;br&gt;Battery management for mobile phone
&lt;br&gt;Electric motor control
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;L X W X H =Length X Width X Height 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KSKE"&gt;https://katalog.we-online.com/en/pbs/WRIS-KSKE&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_5.0X2.5X0.6" package="WRIS-KSKE_2010_5.0X2.5X0.6(LXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_560050350011">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050350011.pdf"/>
<attribute name="IR" value="1.93A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050350011 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE2010R200F304HAATE0000"/>
<attribute name="VALUE" value="0.2Ohm"/>
</technology>
<technology name="_560050350012">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050350012.pdf"/>
<attribute name="IR" value="1.38A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050350012 "/>
<attribute name="PRATED" value="0.75W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE2010R390F304HAATE0000"/>
<attribute name="VALUE" value="0.39Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-KSKE_0402" prefix="R">
<description>&lt;b&gt; WRIS-KSKE Thick Film Resistors
&lt;br&gt;General Purpose Current Sensing
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;General purpose current sensing product series Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 50 mΩ ‒ 10 Ω
&lt;br&gt;Resistance tolerance: ±1 %
&lt;br&gt;Rated Power: 0.125 W ‒ 1 W
&lt;br&gt;TCR: ±100; +200; +250; +300 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155°C
&lt;br&gt;Sizes: 0402 / 0603 / 0805 / 1206 / 2010 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Camera; night vision device
&lt;br&gt;Battery management for mobile phone
&lt;br&gt;Electric motor control

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KSKE"&gt;https://katalog.we-online.com/en/pbs/WRIS-KSKE&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="" package="WRIS-KSKE_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_560050310002">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050310002.pdf"/>
<attribute name="IR" value="0.91A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050310002 "/>
<attribute name="PRATED" value="0.125W"/>
<attribute name="TCR" value="300ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE0402R150F108IAATH0000"/>
<attribute name="VALUE" value="0.15Ohm"/>
</technology>
<technology name="_560050310009">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050310009.pdf"/>
<attribute name="IR" value="0.11A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050310009 "/>
<attribute name="PRATED" value="0.125W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE04020100F108KAATH0000"/>
<attribute name="VALUE" value="10Ohm"/>
</technology>
<technology name="_560050310010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050310010.pdf"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050310010 "/>
<attribute name="PRATED" value="0.125W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE0402R500F108HAATH0000"/>
<attribute name="VALUE" value="0.5Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-KSKE_0603" prefix="R">
<description>&lt;b&gt; WRIS-KSKE Thick Film Resistors
&lt;br&gt;General Purpose Current Sensing
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;General purpose current sensing product series Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 50 mΩ ‒ 10 Ω
&lt;br&gt;Resistance tolerance: ±1 %
&lt;br&gt;Rated Power: 0.125 W ‒ 1 W
&lt;br&gt;TCR: ±100; +200; +250; +300 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155°C
&lt;br&gt;Sizes: 0402 / 0603 / 0805 / 1206 / 2010 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Camera; night vision device
&lt;br&gt;Battery management for mobile phone
&lt;br&gt;Electric motor control
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;L X W X H  =Length X Width X Height
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KSKE"&gt;https://katalog.we-online.com/en/pbs/WRIS-KSKE&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_1.6X0.8X0.45" package="WRIS-KSKE_0603_1.6X0.8X0.45(LXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_560050316001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050316001.pdf"/>
<attribute name="IR" value="1.58A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050316001 "/>
<attribute name="PRATED" value="0.25W"/>
<attribute name="TCR" value="250ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE0603R100F104LAATP0000"/>
<attribute name="VALUE" value="0.1Ohm"/>
</technology>
<technology name="_560050316011">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050316011.pdf"/>
<attribute name="IR" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050316011 "/>
<attribute name="PRATED" value="0.25W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE0603R500F104KAATP0000"/>
<attribute name="VALUE" value="0.5Ohm"/>
</technology>
<technology name="_560050316012">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050316012.pdf"/>
<attribute name="IR" value="0.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050316012 "/>
<attribute name="PRATED" value="0.25W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE06030100F104KAATP0000"/>
<attribute name="VALUE" value="10Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WRIS-KSKE_0805" prefix="R">
<description>&lt;b&gt; WRIS-KSKE Thick Film Resistors
&lt;br&gt;General Purpose Current Sensing
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;General purpose current sensing product series Mounting style: SMT-Chip (standard terminal)
&lt;br&gt;Resistance range: 50 mΩ ‒ 10 Ω
&lt;br&gt;Resistance tolerance: ±1 %
&lt;br&gt;Rated Power: 0.125 W ‒ 1 W
&lt;br&gt;TCR: ±100; +200; +250; +300 ppm/°C
&lt;br&gt;Operating temperature: -55 °C up to +155°C
&lt;br&gt;Sizes: 0402 / 0603 / 0805 / 1206 / 2010 / 2512
&lt;br&gt;Recommended soldering: Reflow soldering

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Camera; night vision device
&lt;br&gt;Battery management for mobile phone
&lt;br&gt;Electric motor control
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;L X W X H =Length X Width X Height 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o135740v209%20Family_WRIS-KSKE.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WRIS-KSKE"&gt;https://katalog.we-online.com/en/pbs/WRIS-KSKE&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-09-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="R"/>
</gates>
<devices>
<device name="_2.0X1.25X0.6" package="WRIS-KSKE_0805_2.0X1.25X0.6(LXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_560050320001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050320001.pdf"/>
<attribute name="IR" value="1.81A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050320001 "/>
<attribute name="PRATED" value="0.33W"/>
<attribute name="TCR" value="250ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE0805R100F103LAATP0000"/>
<attribute name="VALUE" value="0.1Ohm"/>
</technology>
<technology name="_560050320003">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050320003.pdf"/>
<attribute name="IR" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050320003 "/>
<attribute name="PRATED" value="0.33W"/>
<attribute name="TCR" value="200ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE0805R270F103HAATP0000"/>
<attribute name="VALUE" value="0.27Ohm"/>
</technology>
<technology name="_560050320007">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050320007.pdf"/>
<attribute name="IR" value="0.38A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050320007 "/>
<attribute name="PRATED" value="0.33W"/>
<attribute name="TCR" value="100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE08052R20F103KAATP0000"/>
<attribute name="VALUE" value="2.2Ohm"/>
</technology>
<technology name="_560050320011">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/560050320011.pdf"/>
<attribute name="IR" value="0.57A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 560050320011 "/>
<attribute name="PRATED" value="0.33W"/>
<attribute name="TCR" value="±100ppm/ °C"/>
<attribute name="TECHNICAL-REFERENCE" value="KE08051R00F103KAATP0000"/>
<attribute name="VALUE" value="1Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
