<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - IIIuminated Switches - IIIuminated Push Button Switch - WS-PBTL&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-02-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik
7</description>
<packages>
<package name="465M111172501">
<description>&lt;b&gt;WS-PBTL&lt;/b&gt;&lt;br&gt;THT RGB Illuminated Push Button Switch 15 x 15 mm</description>
</package>
<package name="465RG11172501">
<description>&lt;b&gt;WS-PBTL&lt;/b&gt;&lt;br&gt; THT RG Illuminated Push Button Switch 15 x 15 mm</description>
</package>
</packages>
<symbols>
<symbol name="465M111172501">
<description>465M111172501</description>
<pin name="LC" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="L1" direction="pas"/>
<pin name="L2" direction="pas"/>
<pin name="L3" direction="pas"/>
</symbol>
<symbol name="465RG11172501">
<description>465RG11172501</description>
<pin name="LC" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="L1" direction="pas"/>
<pin name="L2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="465M111172501" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-PBTL THT RGB Illuminated Push Button Switch 15 x 15 mm &lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Actuator Flammability Rating:UL94 HB
&lt;br&gt;Actuator Color:White
&lt;br&gt;Actuator Fixture Material:PA66
&lt;br&gt;Actuator Fixture Color:Black
&lt;br&gt;Frame Material:PA66
&lt;br&gt;Frame Flammability Rating:UL94 HB
&lt;br&gt;Frame Color:Black
&lt;br&gt;Stationary Board:PA66
&lt;br&gt;Stationary Board Flammability Rating:UL94 HB
&lt;br&gt;Stationary Board Color:Black
&lt;br&gt;Stationary Contact:Copper Alloy
&lt;br&gt;Stationary Contact Plating:Gold
&lt;br&gt;Moveable Contact Material:Copper Alloy
&lt;br&gt;Moveable Contact Plating:Gold
&lt;br&gt;Spring Material:Carbon Steel
&lt;br&gt;Terminal Material:Copper Alloy
&lt;br&gt;Terminal Plating:Tin
&lt;br&gt;LED Terminal:Copper Alloy
&lt;br&gt;LED Terminal Plating:Tin
&lt;br&gt;IR 1:100 mA
&lt;br&gt;Contact Resistance After Life Test:300 mΩ
&lt;br&gt;RISO:100 MΩ
&lt;br&gt;Withstanding Voltage:500 V (AC)
&lt;br&gt;Function of Push Button:momentary
&lt;br&gt;Actuation Feedback:non-tactile
&lt;br&gt;Schematic:SPST
&lt;br&gt;Qty.:64
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Material Properties:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material:POM
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operation Force 200 g
&lt;br&gt;
&lt;b&gt;General Information:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;
&lt;b&gt;Packaging Properties:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Packaging:ESD Tray
&lt;br&gt;
&lt;b&gt;Ledcolor:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Emitting Color:Red &amp; Green &amp; Blue
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55791v209%20WS-PBTL_Illuminated_THT_Push.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55791v209%20WS-PBTL_Illuminated_THT_Push.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/RGB_PUSH_BUTTON_SWITCH_THT/"&gt;https://www.we-online.com/catalog/en/RGB_PUSH_BUTTON_SWITCH_THT/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun Shan,2020-02-26&lt;br&gt;
&lt;br&gt;2020(C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="465M111172501"/>
</gates>
<devices>
<device name="" package="465M111172501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="L3" pad="L3"/>
<connect gate="G$1" pin="LC" pad="LC"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/465M111172501.pdf"/>
<attribute name="ELECTRICAL-LIFE" value="1000000 times"/>
<attribute name="EMITTING-COLOR" value="Red&amp;Green&amp;Blue"/>
<attribute name="PART-NUMBER" value="465M111172501"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="465RG11172501" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-PBTL THT RG Illuminated Push Button Switch 15 x 15 mm&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PROPERTIES:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Actuator Flammability Rating:UL94 HB
&lt;br&gt;Stationary Board:PA66
&lt;br&gt;Stationary Board Flammability Rating:UL94 HB
&lt;br&gt;Stationary Contact Plating:Gold
&lt;br&gt;Moveable Contact Plating:Gold
&lt;br&gt;Spring Material:Carbon Steel
&lt;br&gt;Terminal Plating:Tin
&lt;br&gt;IR 1:100 mA
&lt;br&gt;RISO:100 MΩ
&lt;br&gt;Withstanding Voltage:500 V (AC)
&lt;br&gt;Qty.:64
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Material Properties:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Actuator Material:POM
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Mechanical Properties:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operation Force 200 g
&lt;br&gt;
&lt;b&gt;General Information:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;
&lt;b&gt;Packaging Properties:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Packaging:ESD Tray
&lt;br&gt;
&lt;b&gt;Ledcolor:&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Emitting Color:Red &amp; Green
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55791v209%20WS-PBTL_Illuminated_THT_Push.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55791v209%20WS-PBTL_Illuminated_THT_Push.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PBTL_PUSH_BUTTON_SWITCH_THT/"&gt;https://www.we-online.com/catalog/en/PBTL_PUSH_BUTTON_SWITCH_THT/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun Shan,2020-02-26&lt;br&gt;
&lt;br&gt;2020(C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="465RG11172501"/>
</gates>
<devices>
<device name="" package="465RG11172501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="LC" pad="LC"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/465RG11172501.pdf"/>
<attribute name="PART-NUMBER" value="465RG11172501"/>
<attribute name="QTY" value="64"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
